{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":18,"n_cols":6,"rows_kept":18,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FAA-B / AZAS-MV1"]
[]
[]
[]
[]
["","","","","FAA71BUV1B / AZAS71M2V1B","FAA100BUV1B / AZAS100M7V1B"]
["Aušinimo galingumas","Nom.","","kW","6.80","9.5"]
["Šildymo galingumas","Nom.","","kW","7.50","10.8"]
["Patalpos vėsinimas","Energijos efektyvumo klasė","","","A+","A"]
["","Vėsinimas","Pdesign","kW","6.80","9.5"]
["","SEER","","","5.77","5.25"]
["","Metinės energijos sąnaudos","","kWh/a","412","633"]
["Patalpos šildymas (vidutinis klimatas)","Energijos efektyvumo klasė","","","A","A"]
["","Pajėgumas","Pdesign","kW","4.50","6"]
["","SCOP/A","","","3.81","3.81"]
["","Metinės energijos sąnaudos","","kWh/a","1654","2205"]
["Pastabos","","","","(1) - Nominalus aušinimo galingumas yra pagrįstas: patalpų temp.: 27°CDB/19°CWB, išorinė temperatūra: 35 °CDB, ekvivalentinis šaltnešio vamzdynas: 5 m, aukščio skirtumas: 0 m.","(1) - Nominalus aušinimo galingumas yra pagrįstas: patalpų temp.: 27°CDB/19°CWB, išorinė temperatūra: 35 °CDB, ekvivalentinis šaltnešio vamzdynas: 5 m, aukščio skirtumas: 0 m."]
["","","","","(2) - Nominali šildymo galia nustatyta remiantis: vidaus temperatūra: 20 °CDB, lauko temperatūra: 7 °CDB, 6 °CWB, ekvivalentinis aušinimo medžiagos vamzdyno ilgis: 5 m, aukščių skirtumas: 0 m.","(2) - Nominali šildymo galia nustatyta remiantis: vidaus temperatūra: 20 °CDB, lauko temperatūra: 7 °CDB, 6 °CWB, ekvivalentinis aušinimo medžiagos vamzdyno ilgis: 5 m, aukščių skirtumas: 0 m."]