{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":26,"n_cols":9,"rows_kept":26,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FAA-B / RZQG-L(8)Y1"]
[]
[]
[]
[]
["","","","","FAA71BUV1B / FAA71BUV1B / RZQG100L8Y1B","FAA71BUV1B / FAA71BUV1B / RZQG125L8Y1B","FAA100BUV1B / RZQG100L8Y1B","FAA71BUV1B / RZQG71L8Y1B","FAA100BUV1B / RZQG71L8Y1B"]
["Aušinimo galingumas","Nom.","","kW","","","","6.80","6.80"]
["Erdvės vėsinimas","SEER","","","","","","6.43","6.43"]
["","Metinės energijos sąnaudos","","kWh/m.","","","","371","371"]
["","Vėsinimas","Pdesign","kW","","","","6.80","6.80"]
["","Energijos efektyvumo klasė","","","","","","A++","A++"]
["Patalpos šildymas (vidutinis klimatas)","Pajėgumas","Pdesign","kW","","","","6.33","6.33"]
["","SCOP/A","","","","","","4.02","4.02"]
["","Energijos efektyvumo klasė","","","","","","A+","A+"]
["","Metinės energijos sąnaudos","","kWh/m.","","","","2,205","2,205"]
["Vardinis našumas","EER","","","","","","3.40","3.40"]
["","Metinis energijos sunaudojimas","","kWh","","","","1,000"]
["","COP","","","","","","3.70"]
["","Energijos suvartojimo ženklinimo direktyva","Vėsinimas","","","","","A"]
["","","Šildymas","","","","","A"]
["Šildymo galingumas","Nom.","","kW","","","","7.50"]
["Energijos naudojimo efektyvumo klasė","","","","A+++ ~ D","A+++ ~ D","A+++ ~ D"]
["Pastabos","","","","","","","(1) - Nominalus aušinimo galingumas yra pagrįstas: patalpų temp.: 27°CDB/19°CWB, išorinė temperatūra: 35 °CDB, ekvivalentinis šaltnešio vamzdynas: 5 m, aukščio skirtumas: 0 m.","(1) - Žr. specialų darbinio diapazono brėžinį"]
["","","","","","","","(2) - Nominali šildymo galia nustatyta remiantis: vidaus temperatūra: 20 °CDB, lauko temperatūra: 7 °CDB, 6 °CWB, ekvivalentinis aušinimo medžiagos vamzdyno ilgis: 5 m, aukščių skirtumas: 0 m.","(2) - Žr. atskirą elektros duomenų brėžinį"]
["","","","","","","","(3) - Žr. specialų darbinio diapazono brėžinį"]
["","","","","","","","(4) - Žr. atskirą elektros duomenų brėžinį"]