{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":41,"n_cols":7,"rows_kept":41,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FAA-B"]
[]
[]
[]
[]
["","","","","","FAA71BUV1B","FAA100BUV1B"]
["Korpusas","Spalva","","","","Balta","Balta"]
["","Medžiaga","","","","Derva","Derva"]
["Matmenys","Įrenginys","","Aukštis","mm","290","340"]
["","","","Plotis","mm","1050","1200"]
["","","","Gylis","mm","269","262"]
["Svoris","Įrenginys","","","kg","14","18"]
["Ventiliatorius","Oro debitas","Aušinimas","Didelis","m³/min.","16.2","23"]
["","Oro srauto greitis","Vėsinimas","Vidutinis","m³/min.","13.4","21.1"]
["","","","Mažas","m³/min.","12.1","18.7"]
["","","Šildymas","Didelis","m³/min.","16.9","23"]
["","Oro srauto greitis","Šildymas","Vidutinis","m³/min.","14.2","20.9"]
["","","Šildymas","Mažas","m³/min.","12.7","18.7"]
["Garso galingumo lygis","Vėsinimas","","","dBA","61","65"]
["","Šildymas","","","dBA","61","65"]
["Garso slėgio lygis","Aušinimas","","Aukštas","dBA","45","49"]
["","Vėsinimas","","Vidutinis","dBA","42","45"]
["","","","Žemas","dBA","40","41"]
["","Šildymas","","Aukštas","dBA","45","49"]
["","","","Vidutinis","dBA","42","45"]
["","","","Žemas","dBA","40","41"]
["Vamzdžių jungtys","Skystis","","OD","mm","9.52","9.52"]
["","Dujos","","Iš. diam.","mm","15.9","15.9"]
["","Drenažas","","","","VP13 (I.D. 13/O.D. 18)","VP13 (I.D. 13/O.D. 18)"]
["El. tiekimas","Fazė","","","","1~","1~"]
["Maitinimas","Dažnis","","","Hz","50","50"]
["","Įtampa","","","V","220-240","220-240"]
["Standartiniai priedai","Installation plate","","","","1","1"]
["","General safety precautions","","","","1","1"]
["","Wire clamp material","","","","4","4"]
["","Heat insulating tape","","","","1","1"]
["","Installation and operation manual","","","","1","1"]
["","Screw bag","","","","1","1"]
["Pastabos","","","","","(1) - Nominalus aušinimo galingumas yra pagrįstas: patalpų temp.: 27°CDB/19°CWB, išorinė temperatūra: 35 °CDB, ekvivalentinis šaltnešio vamzdynas: 5 m, aukščio skirtumas: 0 m."]
["","","","","","(2) - Nominali šildymo galia nustatyta remiantis: vidaus temperatūra: 20 °CDB, lauko temperatūra: 7 °CDB, 6 °CWB, ekvivalentinis aušinimo medžiagos vamzdyno ilgis: 5 m, aukščių skirtumas: 0 m."]
["Standartiniai priedai","Screw cover","","","","","3"]