{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":30,"n_cols":6,"rows_kept":30,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FAQ-C9"]
[]
[]
[]
[]
["","","","","FAQ71CVEB9","FAQ100CVEB9"]
["Garso slėgio lygis","Šildymas","Aukštas","dBA","45","49"]
["","","Nom.","dBA","42","45"]
["","","Vidutinis","dBA","42","45"]
["","","Žemas","dBA","40","41"]
["","Aušinimas","Vidutinis","dBA","42","45"]
["","","Žemas","dBA","40","41"]
["","","Aukštas","dBA","45","49"]
["","","Nom.","dBA","42","45"]
["Aušinimo galingumas","Bendras galingumas","Nom.","kW","0.051","0.061"]
["Vamzdžių jungtys","Skysčių vamzdis","OD","mm","9.52","9.52"]
["","Dujos","Iš. diam.","mm","15.9","15.9"]
["","Drenažo vamzdis","","","VP13 (I.D. 13/O.D. 18)","VP13 (I.D. 13/O.D. 18)"]
["Garso galingumo lygis","Vėsinimas","","dBA","61","65"]
["","Šildymas","","dBA","61","65"]
["Matmenys","Vienetas","Plotis","mm","1,050","1,200"]
["","","Gylis","mm","238","240"]
["","","Aukštis","mm","290","340"]
["Casing","Medžiaga","","","Derva","Derva"]
["","Colour","","","Ryškiai balta","Ryškiai balta"]
["Svoris","Vienetas","","kg","13","17"]
["Šildymo galingumas","Bendras pajėgumas","Nom.","kW","0.068","0.061"]
["Power supply","Fazė","","","1~","1~"]
["","Dažnis","","Hz","50","50"]
["","Įtampa","","V","220-240","220-240"]