{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":27,"n_cols":6,"rows_kept":27,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FBA-A(9) / RXM-A"]
[]
[]
[]
[]
["","","","","FBA50A2VEB9 / RXM50A5V1B","FBA60A2VEB9 / RXM60A5V1B"]
["Aušinimo galingumas","Nom.","","kW","5.0","5.7"]
["Šildymo galingumas","Nom.","","kW","5.5","7"]
["Nominalus efektyvumas","EER","","","3.55","3.48"]
["","COP","","","3.83","3.71"]
["","Metinis energijos sunaudojimas","","kWh","704","819"]
["Vardinis našumas","Energijos suvartojimo ženklinimo direktyva","Vėsinimas","","A","A"]
["","","Šildymas","","A","A"]
["Patalpos vėsinimas","Energijos efektyvumo klasė","","","A++","A+"]
["","Vėsinimas","Pdesign","kW","5.0","5.7"]
["","SEER","","","6.27","5.91"]
["","Metinės energijos sąnaudos","","kWh/a","279","336"]
["Patalpos šildymas (vidutinis klimatas)","Energijos efektyvumo klasė","","","A+","A+"]
["","Pajėgumas","Pdesign","kW","4.4","4.6"]
["","SCOP/A","","","4.06","4.01"]
["","Pdh Šildymo pajėgumas esant –10°","","kW","3.73","3.99"]
["","Metinės energijos sąnaudos","","kWh/a","1,517","1607"]
["Energijos naudojimo efektyvumo klasė","","","","","A+++ ~ D"]
["Pastabos","","","","","(1) - Nominalus aušinimo galingumas yra pagrįstas: patalpų temp.: 27°CDB/19°CWB, išorinė temperatūra: 35 °CDB, ekvivalentinis šaltnešio vamzdynas: 5 m, aukščio skirtumas: 0 m."]
["","","","","","(2) - Nominali šildymo galia nustatyta remiantis: vidaus temperatūra: 20 °CDB, lauko temperatūra: 7 °CDB, 6 °CWB, ekvivalentinis aušinimo medžiagos vamzdyno ilgis: 5 m, aukščių skirtumas: 0 m."]
["","","","","","(3) - Žr. specialų darbinio diapazono brėžinį"]
["","","","","","(4) - Žr. atskirą elektros duomenų brėžinį"]