{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":19,"n_cols":5,"rows_kept":19,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FBA-A / AZAS-MV1"]
[]
[]
[]
[]
["","","","","FBA71A2VEB / AZAS71M2V1B (Archived)"]
["Išorinis įrenginys","","","","AZAS71M2V1B"]
["Aušinimo galingumas","Nom.","","kW","6.80"]
["Šildymo galingumas","Nom.","","kW","7.50"]
["Patalpos vėsinimas","Energijos efektyvumo klasė","","","A"]
["","Vėsinimas","Pdesign","kW","6.80"]
["","SEER","","","5.57"]
["","Metinės energijos sąnaudos","","kWh/a","427"]
["Patalpos šildymas (vidutinis klimatas)","Energijos efektyvumo klasė","","","A"]
["","Pajėgumas","Pdesign","kW","4.50"]
["","SCOP/A","","","3.81"]
["","Metinės energijos sąnaudos","","kWh/a","1654"]
["Pastabos","","","","(1) - Vėsinimas: T2: vidinė temp. 26,6 °CDB, 19,4 °CWB, lauko temp. 48 °CDB [Btu/val./W]"]
["","","","","(2) - Nominali šildymo galia nustatyta remiantis: vidaus temperatūra: 20 °CDB, lauko temperatūra: 7 °CDB, 6 °CWB, ekvivalentinis aušinimo medžiagos vamzdyno ilgis: 5 m, aukščių skirtumas: 0 m."]