{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":40,"n_cols":23,"rows_kept":40,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FBQ-D / RZQG-L9V1"]
[]
[]
[]
[]
["","","","","FBQ100D2VEB / RZQG71L9V1B","FBQ35D2VEB / FBQ35D2VEB / FBQ35D2VEB / RZQG71L9V1B","FBQ35D2VEB / FBQ35D2VEB / RZQG71L9V1B","FBQ50D2VEB / FBQ50D2VEB / RZQG71L9V1B","FBQ100D2VEB / RZQG100L9V1B","FBQ140D2VEB / RZQG100L9V1B","FBQ35D2VEB / FBQ35D2VEB / FBQ35D2VEB / FBQ35D2VEB / RZQG100L9V1B","FBQ35D2VEB / FBQ35D2VEB / FBQ35D2VEB / RZQG100L9V1B","FBQ50D2VEB / FBQ50D2VEB / FBQ50D2VEB / RZQG100L9V1B","FBQ50D2VEB / FBQ50D2VEB / RZQG100L9V1B","FBQ71D2VEB / FBQ71D2VEB / RZQG100L9V1B","FBQ140D2VEB / RZQG125L9V1B","FBQ35D2VEB / FBQ35D2VEB / FBQ35D2VEB / FBQ35D2VEB / RZQG125L9V1B","FBQ50D2VEB / FBQ50D2VEB / FBQ50D2VEB / RZQG125L9V1B","FBQ71D2VEB / FBQ71D2VEB / RZQG125L9V1B","FBQ140D2VEB / RZQG140L9V1B","FBQ71D2VEB / RZQG71L9V1B (Archived)","FBQ60D2VEB / FBQ60D2VEB / RZQG125L9V1B (Archived)","FBQ125D2VEB / RZQG125L9V1B (Archived)"]
["Aušinimo galingumas","Nom.","","kW","","","","","9.5 (2)","","","","","","","","","","","13.4 (2)"]
["Erdvės vėsinimas","SEER","","","6.16","5.10","5.10","5.10","5.87","5.87","5.10","5.10","5.10","5.10","5.10","6.11","5.10","5.10","5.10"]
["","Metinės energijos sąnaudos","","kWh/m.","386","466","466","466","566","566","652","652","652","652","652","687","824","824","824"]
["","Vėsinimas","Pdesign","kW","6.80","6.80","6.80","6.80","9.50","9.50","9.50","9.50","9.50","9.50","9.50","12.00","12.00","12.00","12.00"]
["","Energijos efektyvumo klasė","","","A++","A","A","A","A+","A+","A","A","A","A","A","A++","A","A","A"]
["Patalpos šildymas (vidutinis klimatas)","Pajėgumas","Pdesign","kW","6.00","6.00","6.00","6.00","11.30","11.30","11.30","11.30","11.30","11.30","11.30","12.70","12.71","12.71","12.71"]
["","SCOP/A","","","4.31","3.80","3.80","3.80","4.78","4.78","3.80","3.80","3.80","3.80","3.80","4.28","3.80","3.80","3.80"]
["","Energijos efektyvumo klasė","","","A+","A","A","A","A++","A++","A","A","A","A","A","A+","A","A","A"]
["","Metinės energijos sąnaudos","","kWh/m.","1,949","2,210","2,210","2,210","3,310","3,310","4,163","4,163","4,163","4,163","4,163","4,154","4,683","4,683","4,683"]
["Vardinis našumas","Metinis energijos sunaudojimas","","kWh","","","","","1,247"]
["","EER","","","","","","","3.81 (1)","","","","","","","","","","","3.35 (1)"]
["","COP","","","","","","","4.41 (1)","","","","","","","","","","","3.60 (1)"]
["","Energijos suvartojimo ženklinimo direktyva","Vėsinimas","","","","","","A"]
["","","Šildymas","","","","","","A"]
["Šildymo galingumas","Nom.","","kW","","","","","10.80 (2)","","","","","","","","","","","15.50 (2)"]
["Pastabos","","","","","","","","(1) - EER/COP pagal „Eurovent 2012“, skirta naudoti tik už ES ribų","","","","","","","","","","","(1) - EER/COP pagal „Eurovent 2012“, skirta naudoti tik už ES ribų","(1) - EER/COP pagal „Eurovent 2012“, skirta naudoti tik už ES ribų","","(1) - EER/COP pagal „Eurovent 2012“, skirta naudoti tik už ES ribų"]
["","","","","","","","","(2) - Nominalus efektyvumas: vėsinimas esant 35°/27° nominaliąja apkrova, šildymas esant 7°/20° nominaliąja apkrova","","","","","","","","","","","(2) - Nominalus efektyvumas: vėsinimas esant 35°/27° nominaliąja apkrova, šildymas esant 7°/20° nominaliąja apkrova","(2) - Nominalus efektyvumas: vėsinimas esant 35°/27° nominaliąja apkrova, šildymas esant 7°/20° nominaliąja apkrova","","(2) - Nominalus efektyvumas: vėsinimas esant 35°/27° nominaliąja apkrova, šildymas esant 7°/20° nominaliąja apkrova"]
["","","","","","","(1) - EER/COP pagal „Eurovent 2012“, skirta naudoti tik už ES ribų","","","","","(1) - EER/COP pagal „Eurovent 2012“, skirta naudoti tik už ES ribų","","(1) - EER/COP pagal „Eurovent 2012“, skirta naudoti tik už ES ribų","","","","","","","","(1) - EER/COP pagal „Eurovent 2012“, skirta naudoti tik už ES ribų"]
["Išorinis įrenginys","","","","","","","","","","","","","","","","","","","","RZQG71L9V1","RZQG125L9V1","RZQG125L9V1"]
["Aušinimo galingumas","Nom.","","kW","","","","","","","","","","","","","","","","","6.8","","12.0"]
["Šildymo galingumas","Nom.","","kW","","","","","","","","","","","","","","","","","7.5","","13.5"]
["Nominalus efektyvumas","EER","","","","","","","","","","","","","","","","","","","3.53","","3.83"]
["","COP","","","","","","","","","","","","","","","","","","","3.96","","3.83"]
["","Metinis energijos sunaudojimas","","kWh","","","","","","","","","","","","","","","","","963","","1567"]
["Vardinis našumas","Energijos suvartojimo ženklinimo direktyva","Vėsinimas","","","","","","","","","","","","","","","","","","A","","A"]
["","","Šildymas","","","","","","","","","","","","","","","","","","A","","A"]
["Patalpos vėsinimas","Energijos efektyvumo klasė","","","","","","","","","","","","","","","","","","","A++","A","A+"]
["","Vėsinimas","Pdesign","kW","","","","","","","","","","","","","","","","","6.80","12.00","12.00"]
["","SEER","","","","","","","","","","","","","","","","","","","6.16","5.10","5.83"]
["","Metinės energijos sąnaudos","","kWh/m.","","","","","","","","","","","","","","","","","386","824","720"]
["Patalpos šildymas (vidutinis klimatas)","Energijos efektyvumo klasė","","","","","","","","","","","","","","","","","","","A+","A","A+"]
["","Pajėgumas","Pdesign","kW","","","","","","","","","","","","","","","","","6.00","12.71","12.70"]
["","SCOP/A","","","","","","","","","","","","","","","","","","","4.35","3.80","4.37"]
["","Metinės energijos sąnaudos","","kWh/m.","","","","","","","","","","","","","","","","","1931","4683","4069"]