{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":19,"n_cols":8,"rows_kept":19,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FCAG-A / AZAS-MV1"]
[]
[]
[]
[]
["","","","","FCAG100AVEB / AZAS100M7V1B","FCAG71AVEB / AZAS71M2V1B","FCAG125AVEB / AZAS125M7V1B","FCAG140AVEB / AZAS140M7V1B"]
["Aušinimo galingumas","Nom.","","kW","","6.80 (1)","12.1 (1)","13.4 (1)"]
["Šildymo galingumas","Nom.","","kW","","7.50 (2)","13.5 (2)","15.5 (2)"]
["Space cooling","Energijos efektyvumo klasė","","","","A+"]
["","Vėsinimas","Pdesign","kW","","6.80","12.1","13.0"]
["","SEER","","","","5.87","5.40","6.00"]
["","Metinės energijos sąnaudos","","kWh/a","","405","1,345","1,300"]
["Patalpos šildymas (vidutinis klimatas)","Energijos efektyvumo klasė","","","","A"]
["","Pajėgumas","Pdesign","kW","","4.50","6.00","7.80"]
["","SCOP/A","","","","4.00","3.80","4.31"]
["","Metinės energijos sąnaudos","","kWh/a","","1,575","2,211","2,534"]
["Pastabos","","","","","(1) - Vėsinimas: T2: vidinė temp. 26,6 °CDB, 19,4 °CWB, lauko temp. 48 °CDB [Btu/val./W]","(1) - Aušinimas: vidaus temp. 27 °CDB, 19,0 °CWB; lauko temp. 35 °CDB; ekvivalentinis vamzdyno ilgis: 5 m; aukščių skirtumas: 0 m","(1) - Aušinimas: vidaus temp. 27 °CDB, 19,0 °CWB; lauko temp. 35 °CDB; ekvivalentinis vamzdyno ilgis: 5 m; aukščių skirtumas: 0 m"]
["","","","","","(2) - Nominali šildymo galia nustatyta remiantis: vidaus temperatūra: 20 °CDB, lauko temperatūra: 7 °CDB, 6 °CWB, ekvivalentinis aušinimo medžiagos vamzdyno ilgis: 5 m, aukščių skirtumas: 0 m.","(2) - Nominali šildymo galia nustatyta remiantis: vidaus temperatūra: 20 °CDB, lauko temperatūra: 7 °CDB, 6 °CWB, ekvivalentinis aušinimo medžiagos vamzdyno ilgis: 5 m, aukščių skirtumas: 0 m.","(2) - Nominali šildymo galia nustatyta remiantis: vidaus temperatūra: 20 °CDB, lauko temperatūra: 7 °CDB, 6 °CWB, ekvivalentinis aušinimo medžiagos vamzdyno ilgis: 5 m, aukščių skirtumas: 0 m."]
["Energijos naudojimo efektyvumo klasė","","","","A+++ ~ D"]