{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":12,"n_cols":7,"rows_kept":12,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FCAG-A / RR-BW1"]
[]
[]
[]
[]
["","","","","FCAG71AVEB / RR71B8W1B","FCAG100AVEB / RR100B8W1B","FCAG125AVEB / RR125B8W1B"]
["Aušinimo galingumas","Nom.","","kW","7.10 (1)","10.0 (1)","12.5 (1)"]
["Vardinis našumas","EER","","","2.70","2.81","2.69"]
["","Metinis energijos sunaudojimas","","kWh","1,315","1,780","2,325"]
["","Energijos suvartojimo ženklinimo direktyva","Vėsinimas","","D","C","D"]
["Pastabos","","","","(1) - Aušinimas: vidaus temp. 27 °CDB, 19,0 °CWB; lauko temp. 35 °CDB; ekvivalentinis vamzdyno ilgis: 5 m; aukščių skirtumas: 0 m","(1) - Aušinimas: vidaus temp. 27 °CDB, 19,0 °CWB; lauko temp. 35 °CDB; ekvivalentinis vamzdyno ilgis: 5 m; aukščių skirtumas: 0 m","(1) - Aušinimas: vidaus temp. 27 °CDB, 19,0 °CWB; lauko temp. 35 °CDB; ekvivalentinis vamzdyno ilgis: 5 m; aukščių skirtumas: 0 m"]
["","","","","(2) - Šildymas: vidaus temp. 20 °CDB; lauko temp. 7 °CDB, 6 °CWB; ekvivalentinis aušinimo medžiagos vamzdyno ilgis: 5 m; aukščių skirtumas: 0 m","(2) - Šildymas: vidaus temp. 20 °CDB; lauko temp. 7 °CDB, 6 °CWB; ekvivalentinis aušinimo medžiagos vamzdyno ilgis: 5 m; aukščių skirtumas: 0 m","(2) - Šildymas: vidaus temp. 20 °CDB; lauko temp. 7 °CDB, 6 °CWB; ekvivalentinis aušinimo medžiagos vamzdyno ilgis: 5 m; aukščių skirtumas: 0 m"]