{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":19,"n_cols":5,"rows_kept":19,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FCAG-B / ARXM-N9"]
[]
[]
[]
[]
["","","","","FCAG71BVEB / ARXM71N2V1B9"]
["Aušinimo galingumas","Nom.","","kW","6.80"]
["","Maks.","","kW","7.05"]
["Šildymo galingumas","Nom.","","kW","7.50"]
["","Maks.","","kW","7.58"]
["Vardinis našumas","Metinis energijos sunaudojimas","","kWh","1,083"]
["","COP","","","3.38"]
["","EER","","","3.14"]
["","Energijos suvartojimo ženklinimo direktyva","Vėsinimas","","B"]
["","","Šildymas","","C"]
["Pastabos","","","","(1) - Žr. specialų darbinio diapazono brėžinį"]
["","","","","(2) - Žr. atskirą elektros duomenų brėžinį"]
["","","","","(3) - Nominalus aušinimo galingumas yra pagrįstas: patalpų temp.: 27°CDB/19°CWB, išorinė temperatūra: 35 °CDB, ekvivalentinis šaltnešio vamzdynas: 5 m, aukščio skirtumas: 0 m."]
["","","","","(4) - Nominali šildymo galia nustatyta remiantis: vidaus temperatūra: 20 °CDB, lauko temperatūra: 7 °CDB, 6 °CWB, ekvivalentinis aušinimo medžiagos vamzdyno ilgis: 5 m, aukščių skirtumas: 0 m."]