{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":37,"n_cols":13,"rows_kept":37,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FCAHG-G / RZQG-L(8)Y1"]
[]
[]
[]
[]
["","","","","FCAHG100GVEB / RZQG100L8Y1B","FCAHG125GVEB / RZQG125L8Y1B","FCAHG140GVEB / RZQG100L8Y1B","FCAHG140GVEB / RZQG125L8Y1B","FCAHG100GVEB / RZQG71L8Y1B","FCAHG71GVEB / RZQG71L8Y1B","FCAHG71GVEB / FCAHG71GVEB / RZQG100L8Y1B","FCAHG71GVEB / FCAHG71GVEB / RZQG125L8Y1B","FCAHG140GVEB / RZQG140L7Y1B"]
["Aušinimo galingumas","Nom.","","kW","","","","","","6.80 (1)","","","13.4 (1)"]
["Patalpos vėsinimas","SEER","","","","","","","6.91","6.91","","","6.75"]
["","ηs,c","","%","","","","","","","","","266.9"]
["","Metinės energijos sąnaudos","","kWh/a","","","","","345","345","","","1,191"]
["","Vėsinimas","Pdesign","kW","","","","","6.80","6.80","","","13.4"]
["","Energijos efektyvumo klasė","","","","","","","A++","A++"]
["Patalpos šildymas (vidutinis klimatas)","Pajėgumas","Pdesign","kW","","","","","7.60","7.60","","","11.8"]
["","SCOP/A","","","","","","","4.54","4.54","","","4.38"]
["","Energijos efektyvumo klasė","","","","","","","A+","A+"]
["","Metinės energijos sąnaudos","","kWh/a","","","","","2,344","2,344","","","3,766"]
["","ηs,h","","%","","","","","","","","","172.1"]
["Vardinis našumas","Metinis energijos sunaudojimas","","kWh","","","","","","830"]
["","EER","","","","","","","","4.09 (3)","","","3.18 (3)"]
["","COP","","","","","","","","4.80 (3)","","","4.12 (3)"]
["","Energijos suvartojimo ženklinimo direktyva","Vėsinimas","","","","","","","A"]
["","","Šildymas","","","","","","","A"]
["Šildymo galingumas","Nom.","","kW","","","","","","7.50 (2)","","","15.5 (2)"]
["Energijos naudojimo efektyvumo klasė","","","","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","","","A+++ ~ D","A+++ ~ D"]
["Pastabos","","","","","","","","","(1) - Aušinimas: vidaus temp. 27 °CDB, 19 °CWB; lauko temp. 35 °CDB; ekvivalentinis vamzdyno ilgis: 7,5 m; aukščių skirtumas: 0 m","","","(1) - Aušinimas: vidaus temp. 27 °CDB, 19 °CWB; lauko temp. 35 °CDB; ekvivalentinis vamzdyno ilgis: 7,5 m; aukščių skirtumas: 0 m"]
["","","","","","","","","","(2) - Šildymas: vidaus temp. 20 °CDB; lauko temp. 7 °CDB, 6 °CWB; ekvivalentinis aušinimo medžiagos vamzdyno ilgis: 7,5 m; aukščių skirtumas: 0 m","","","(2) - Šildymas: vidaus temp. 20 °CDB; lauko temp. 7 °CDB, 6 °CWB; ekvivalentinis aušinimo medžiagos vamzdyno ilgis: 7,5 m; aukščių skirtumas: 0 m"]
["","","","","","","","","","(3) - EER/COP pagal „Eurovent 2012“, skirta naudoti tik už ES ribų","","","(3) - EER/COP pagal „Eurovent 2012“, skirta naudoti tik už ES ribų"]
["Išorinis įrenginys","","","","","","","","","","RZQG100L8Y1","RZQG125L8Y1"]
["Patalpos vėsinimas","Energijos efektyvumo klasė","","","","","","","","","A","A"]
["","Vėsinimas","Pdesign","kW","","","","","","","9.50","12.0"]
["","SEER","","","","","","","","","5.10","5.10"]
["","Metinės energijos sąnaudos","","kWh/a","","","","","","","652","824"]
["Patalpos šildymas (vidutinis klimatas)","Energijos efektyvumo klasė","","","","","","","","","A","A"]
["","Pajėgumas","Pdesign","kW","","","","","","","11.30","12.71"]
["","SCOP/A","","","","","","","","","3.80","3.80"]
["","Pdh Šildymo pajėgumas esant –10°","","kW","","","","","","","9.66","11.4"]
["","Metinės energijos sąnaudos","","kWh/a","","","","","","","4164","4683"]