{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":24,"n_cols":21,"rows_kept":24,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FCQG-F / RZQG-L(8)Y1"]
[]
[]
[]
[]
["","","","","FCQG100FVEB / RZQG71L8Y1B","FCQG35FVEB / FCQG35FVEB / RZQG71L8Y1B","FCQG71FVEB / RZQG71L8Y1B","FCQG100FVEB / RZQG100L8Y1B","FCQG140FVEB / RZQG100L8Y1B","FCQG35FVEB / FCQG35FVEB / FCQG35FVEB / FCQG35FVEB / RZQG100L8Y1B","FCQG35FVEB / FCQG35FVEB / FCQG35FVEB / RZQG100L8Y1B","FCQG50FVEB / FCQG50FVEB / FCQG50FVEB / RZQG100L8Y1B","FCQG50FVEB / FCQG50FVEB / RZQG100L8Y1B","FCQG71FVEB / FCQG71FVEB / RZQG100L8Y1B","FCQG125FVEB / RZQG125L8Y1B","FCQG140FVEB / RZQG125L8Y1B","FCQG35FVEB / FCQG35FVEB / FCQG35FVEB / FCQG35FVEB / RZQG125L8Y1B","FCQG50FVEB / FCQG50FVEB / FCQG50FVEB / RZQG125L8Y1B","FCQG60FVEB / FCQG60FVEB / RZQG125L8Y1B","FCQG71FVEB / FCQG71FVEB / RZQG125L8Y1B","FCQG140FVEB / RZQG140L7Y1B"]
["Aušinimo galingumas","Nom.","","kW","","","6.8","9.5","","","","","","","12.0","","","","","","13.4"]
["Patalpos vėsinimas","SEER","","","6.80","5.1","6.72","6.8","6.80","5.10","5.1","5.10","5.1","5.10","6","6.00","5.10","5.10","5.1","5.10"]
["","Metinės energijos sąnaudos","","kWh/a","350","467","355","489","489","652","652","652","652","652","700","700","824","824","824","824"]
["","Vėsinimas","Pdesign","kW","6.80","6.8","6.80","9.5","9.50","9.50","9.5","9.50","9.5","9.50","12","12.00","12.00","12.00","12","12.00"]
["","Energijos efektyvumo klasė","","","A++","B","A++","A++","A++","B","B","B","B","B","A+","A+","B","B","B","B"]
["Patalpos šildymas (vidutinis klimatas)","Pajėgumas","Pdesign","kW","6.33","6","6.33","11.3","11.30","11.30","11.3","11.30","11.3","11.30","12.66","12.66","12.71","12.71","12.71","12.71"]
["","SCOP/A","","","4.20","3.8","4.20","4.61","4.61","3.80","3.8","3.80","3.8","3.80","4.1","4.10","3.80","3.80","3.8","3.80"]
["","Energijos efektyvumo klasė","","","A+","A","A+","A++","A++","A","A","A","A","A","A+","A+","A","A","A","A"]
["","Metinės energijos sąnaudos","","kWh/a","2,110","2,211","2,110","3,432","3,432","4,164","4,164","4,164","4,164","4,164","4,323","4,323","4,683","4,683","4,683","4,683"]
["Vardinis našumas","Metinis energijos sunaudojimas","","kWh","","","1,005","1,225","","","","","","","1,610"]
["","EER","","","","","3.39","3.87","","","","","","","3.73","","","","","","3.21"]
["","COP","","","","","3.97","4.15","","","","","","","3.63","","","","","","3.61"]
["","Energijos suvartojimo ženklinimo direktyva","Vėsinimas","","","","A","A","","","","","","","A"]
["","","Šildymas","","","","A","A","","","","","","","A"]
["Šildymo galingumas","Nom.","","kW","","","7.5","10.8","","","","","","","13.5","","","","","","15.5"]
["Pastabos","","","","","","(1) - Metinės energijos sąnaudos pagal energijos žymėjimo direktyvą 2002/31/EB","(1) - EER/COP pagal „Eurovent 2012“, skirta naudoti tik už ES ribų","","","","","","","(1) - EER/COP pagal „Eurovent 2012“, skirta naudoti tik už ES ribų","","","","","","(1) - EER/COP pagal „Eurovent 2012“, skirta naudoti tik už ES ribų"]
["","","","","","","(2) - SEER ir SCOP pagal EN 14825","(2) - Nominalus efektyvumas: vėsinimas esant 35°/27° nominaliąja apkrova, šildymas esant 7°/20° nominaliąja apkrova","","","","","","","(2) - Nominalus efektyvumas: vėsinimas esant 35°/27° nominaliąja apkrova, šildymas esant 7°/20° nominaliąja apkrova","","","","","","(2) - Nominalus efektyvumas: vėsinimas esant 35°/27° nominaliąja apkrova, šildymas esant 7°/20° nominaliąja apkrova"]
["","","","","","(1) - EER/COP pagal „Eurovent 2012“, skirta naudoti tik už ES ribų","","","","","(1) - EER/COP pagal „Eurovent 2012“, skirta naudoti tik už ES ribų","","(1) - EER/COP pagal „Eurovent 2012“, skirta naudoti tik už ES ribų","","","","","","(1) - EER/COP pagal „Eurovent 2012“, skirta naudoti tik už ES ribų"]