{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":23,"n_cols":8,"rows_kept":23,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FCQHG-F / RZQSG-L3/9V1"]
[]
[]
[]
[]
["","","","","FCQHG71FVEB / RZQSG71L3V1B","FCQHG100FVEB / RZQSG100L9V1B","FCQHG125FVEB / RZQSG125L9V1B","FCQHG140FVEB / RZQSG140L9V1B"]
["Aušinimo galingumas","Nom.","","kW","6.8","9.5","12.0","13.4"]
["Erdvės vėsinimas","SEER","","","6.50","6.70","5.40"]
["","Metinės energijos sąnaudos","","kWh/m.","366","497","778"]
["","Vėsinimas","Pdesign","kW","6.80","9.50","12.00"]
["","Energijos efektyvumo klasė","","","A++","A++","A"]
["Patalpos šildymas (vidutinis klimatas)","Pajėgumas","Pdesign","kW","7.60","8.03","8.03"]
["","SCOP/A","","","4.15","4.30","4.10"]
["","Energijos efektyvumo klasė","","","A+","A+","A+"]
["","Metinės energijos sąnaudos","","kWh/m.","2,563","2,615","2,742"]
["Vardinis našumas","Metinis energijos sunaudojimas","","kWh","970","1,285","1,855"]
["","EER","","","3.50","3.70","3.23","3.21"]
["","COP","","","4.10","4.30","3.75","3.61"]
["","Energijos suvartojimo ženklinimo direktyva","Vėsinimas","","A","A","A"]
["","","Šildymas","","A","A","A"]
["Šildymo galingumas","Nom.","","kW","7.5","10.8","13.5","15.5"]
["Pastabos","","","","(1) - EER/COP pagal „Eurovent 2012“, skirta naudoti tik už ES ribų","(1) - EER/COP pagal „Eurovent 2012“, skirta naudoti tik už ES ribų","(1) - EER/COP pagal „Eurovent 2012“, skirta naudoti tik už ES ribų","(1) - EER/COP pagal „Eurovent 2012“, skirta naudoti tik už ES ribų"]
["","","","","(2) - Nominalus efektyvumas: vėsinimas esant 35°/27° nominaliąja apkrova, šildymas esant 7°/20° nominaliąja apkrova","(2) - Nominalus efektyvumas: vėsinimas esant 35°/27° nominaliąja apkrova, šildymas esant 7°/20° nominaliąja apkrova","(2) - Nominalus efektyvumas: vėsinimas esant 35°/27° nominaliąja apkrova, šildymas esant 7°/20° nominaliąja apkrova","(2) - Nominalus efektyvumas: vėsinimas esant 35°/27° nominaliąja apkrova, šildymas esant 7°/20° nominaliąja apkrova"]