{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":17,"n_cols":6,"rows_kept":17,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDA-A / RZAG-NV1"]
[]
[]
[]
[]
["","","","","FDA125A5VEB / RZAG125N2V1B","FDA125A5VEB / RZAG125N7V1B"]
["Aušinimo galingumas","Nom.","","kW","12.1 (1)","12.1 (1)"]
["Šildymo galingumas","Nom.","","kW","13.5 (2)","13.5 (2)"]
["Patalpos vėsinimas","Vėsinimas","Pdesign","kW","12.1","12.1"]
["","SEER","","","6.59","6.59"]
["","Metinės energijos sąnaudos","","kWh/m.","1102","1102"]
["Patalpos šildymas (vidutinis klimatas)","Pajėgumas","Pdesign","kW","9.52","9.52"]
["","SCOP/A","","","4.35","4.35"]
["","Metinės energijos sąnaudos","","kWh/m.","3064","3064"]
["Energijos naudojimo efektyvumo klasė","","","","A+++ ~ D","A+++ ~ D"]
["Pastabos","","","","(1) - Nominalus aušinimo galingumas yra pagrįstas: patalpų temp.: 27°CDB/19°CWB, išorinė temperatūra: 35 °CDB, ekvivalentinis šaltnešio vamzdynas: 5 m, aukščio skirtumas: 0 m.","(1) - Nominalus aušinimo galingumas yra pagrįstas: patalpų temp.: 27°CDB/19°CWB, išorinė temperatūra: 35 °CDB, ekvivalentinis šaltnešio vamzdynas: 5 m, aukščio skirtumas: 0 m."]
["","","","","(2) - Nominali šildymo galia nustatyta remiantis: vidaus temperatūra: 20 °CDB, lauko temperatūra: 7 °CDB, 6 °CWB, ekvivalentinis aušinimo medžiagos vamzdyno ilgis: 5 m, aukščių skirtumas: 0 m.","(2) - Nominali šildymo galia nustatyta remiantis: vidaus temperatūra: 20 °CDB, lauko temperatūra: 7 °CDB, 6 °CWB, ekvivalentinis aušinimo medžiagos vamzdyno ilgis: 5 m, aukščių skirtumas: 0 m."]