{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":18,"n_cols":5,"rows_kept":18,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDA-A / RZASG-MY1"]
[]
[]
[]
[]
["","","","","FDA125A5VEB / RZASG125M7Y1B"]
["Aušinimo galingumas","Nom.","","kW","12.1 (1)"]
["Šildymo galingumas","Nom.","","kW","13.5 (2)"]
["Erdvės vėsinimas","Vėsinimas","Pdesign","kW","12.1"]
["","SEER","","","5.03"]
["","Metinės energijos sąnaudos","","kWh/m.","1,444"]
["Patalpos šildymas (vidutinis klimatas)","Pajėgumas","Pdesign","kW","6.00"]
["","SCOP/A","","","3.58"]
["","Metinės energijos sąnaudos","","kWh/m.","2,346"]
["Pastabos","","","","(1) - Nominalus aušinimo galingumas yra pagrįstas: patalpų temp.: 27°CDB/19°CWB, išorinė temperatūra: 35 °CDB, ekvivalentinis šaltnešio vamzdynas: 5 m, aukščio skirtumas: 0 m."]
["","","","","(2) - Nominali šildymo galia nustatyta remiantis: vidaus temperatūra: 20 °CDB, lauko temperatūra: 7 °CDB, 6 °CWB, ekvivalentinis aušinimo medžiagos vamzdyno ilgis: 5 m, aukščių skirtumas: 0 m."]
["","","","","(3) - Žr. specialų darbinio diapazono brėžinį"]
["","","","","(4) - Žr. atskirą elektros duomenų brėžinį"]