{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":67,"n_cols":8,"rows_kept":67,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDA-A"]
[]
[]
[]
[]
["","","","","","FDA125A5VEB","FDA200AXVEB","FDA250AXVEB"]
["Aušinimo galingumas","Bendras pajėgumas","","Nom.","kW","12.10","19.00","22.00"]
["Šildymo galingumas","Bendras pajėgumas","","Nom.","kW","13.50","22.4","24.0"]
["Korpusas","Spalva","","","","Nedažytas","Nedažytas","Nedažytas"]
["","Medžiaga","","","","Galvanizuotas plienas","Galvanizuoto plieno plokštė","Galvanizuoto plieno plokštė"]
["Matmenys","Įrenginys","","Aukštis","mm","300","470","470"]
["","","","Plotis","mm","1,400","1,490","1,490"]
["","","","Gylis","mm","700","1,100","1,100"]
["Svoris","Įrenginys","","","kg","45","104","115"]
["Reikiama anga lubose >","mm","","","","350"]
["Ventiliatorius","Oro debitas","Aušinimas","Didelis","m³/min.","39.0","64.0","69.0"]
["","","","Vidutinis","m³/min.","","50","56"]
["","","","Mažas","m³/min.","28.0","36.0","43.0"]
["","","Šildymas","Didelis","m³/min.","39.0","64.0","69.0"]
["","","","Vidutinis","m³/min.","","50.0","56.0"]
["","","","Mažas","m³/min.","28.0","36.0","43.0"]
["","Išorinis statinis slėgis","","Aukštas","Pa","200","250","250"]
["","","","Nom.","Pa","50","62","62"]
["Sound power level","Vėsinimas","","","dBA","66","69.0","71.0"]
["Garso slėgio lygis","Aušinimas","","Aukštas","dBA","40","43.0","44.0"]
["","","","Vidutinis","dBA","","39.0","40.0"]
["","","","Žemas","dBA","33","36.0","37.0"]
["","Šildymas","","Aukštas","dBA","40","43.0","44.0"]
["","","","Vidutinis","dBA","","39.0","40.0"]
["","","","Žemas","dBA","33","36.0","37.0"]
["Vamzdžių jungtys","Skystis","","OD","mm","9.52","9.52","9.52"]
["","Dujos","","Iš. diam.","mm","15.90","19.1","22.2"]
["","Drenažo vamzdis","","","","VP25 (I.D. 25/O.D. 32)","BSP1","BSP1"]
["Drenavimo aukštis","mm","","","","625"]
["Dekoratyvinis skydelis","Modelis","","","","BYBS125DJW1"]
["","Spalva","","","","Balta spalva (10Y9/0.5)"]
["","Matmenys","","Aukštis","mm","55"]
["","","","Plotis","mm","1,500"]
["","","","Gylis","mm","500"]
["","Svoris","","","kg","6.5"]
["Valdymo sistemos","Infrared remote control","","","","BRC4C65, BRC4C66"]
["","Laidinis nuotolinio valdymo pultelis","","","","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52"]
["Standartiniai priedai","Varžtai","","","","16","2","2"]
["","Poveržlė","","","","8","12","12"]
["","Žarnos juosta","","","","1"]
["","Drenavimo žarna","","","","1"]
["","Bendrosios saugos priemonės","","","","1","1","1"]
["","Montavimo ir eksploatavimo vadovas","","","","1","1","1"]
["","Bendrojo energijos tiekimo laidas","","","","2"]
["","Sandarinimo medžiaga (išleidimo žarna)","","","","1"]
["","Sandarinimo medžiaga","","","","2"]
["","Terminės izoliacijos vamzdis (skysčio)","","","","1"]
["","Terminės izoliacijos vamzdis (dujų)","","","","1"]
["Power supply","Pavadinimas","","","","","VE","VE"]
["","Fazė","","","","1~","1~","1~"]
["","Dažnis","","","Hz","50/60","50/60","50/60"]
["","Įtampa","","","V","220-240/220","220-240/220","220-240/220"]
["Pastabos","","","","","(1) - Žr. atskirą elektros duomenų brėžinį"]
["Standartiniai priedai","Eksploatavimo vadovas","","","","","1","1"]
["","Įrengimo vadovas","","","","","1","1"]
["","Dujas jungiantis vamzdis","","","","","1","1"]
["","Vielinio spaustuko medžiaga","","","","","1","1"]
["","Spyruoklinė poveržlė","","","","","2","2"]
["","Varžtas ir poveržlė","","","","","45","45"]
["","Šešiakampės galvutės varžtas su poveržle","","","","","49","49"]
["","Šešiakampės galvutės varžtas","","","","","2","2"]
["","Paprastoji poveržlė","","","","","8","8"]