{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":37,"n_cols":7,"rows_kept":37,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDBQ-B"]
[]
[]
[]
[]
["","","","","","FDBQ25B5V1","FDBQ25B8V1"]
["Garso slėgio lygis","Šildymas","","Aukštas","dBA","35.0","35.0"]
["","","","Žemas","dBA","29.0","29.0"]
["","Aušinimas","","Žemas","dBA","28.0","28.0"]
["","","","Aukštas","dBA","35.0","35.0"]
["Standartiniai priedai","Montavimo ir eksploatavimo vadovas","","","","1","1"]
["","Įsiurbimo oro filtras","","","","1","1"]
["Control systems","Wired remote control","","","","BRC1D52, BRC1E52A/B"]
["Vamzdžių jungtys","Liquid","","OD","mm","6.35"]
["","Dujos","","Iš. diam.","mm","9.52"]
["","Drenažo vamzdis","","","","27.2"]
["Sound power level","Vėsinimas","","","dBA","55","55"]
["","Šildymas","","","dBA","55","55"]
["Matmenys","Vienetas","","Plotis","mm","652","652"]
["","","","Gylis","mm","502","502"]
["","","","Aukštis","mm","230","230"]
["Korpusas","Material","","","","Galvanizuotas mažai anglies turintis plienas","Galvanizuotas mažai anglies turintis plienas"]
["Svoris","Vienetas","","","kg","17.0","17.0"]
["Fan","Oro debitas","Šildymas","Didelis","m³/min.","","6.95"]
["","","","Mažas","m³/min.","","5.20"]
["","","Aušinimas","Mažas","m³/min.","","5.20"]
["","","","Didelis","m³/min.","","6.50"]
["Power supply","Fazė","","","","1~","1~"]
["","Dažnis","","","Hz","50","50"]
["","Pavadinimas","","","","V1","V1"]
["","Įtampa","","","V","230","230 +/-10%"]
["Pastabos","","","","","(1) - Garso reikšmės yra matuojamos pusiau beaidėje patalpoje.","(1) - Garso reikšmės yra matuojamos pusiau beaidėje patalpoje."]
["","","","","","(2) - Garso slėgio lygis yra santykinė reikšmė, priklausanti nuo atstumo ir akustinės aplinkos. Daugiau informacijos žr. garso lygio diagramose.","(2) - Garso slėgio lygis yra santykinė reikšmė, priklausanti nuo atstumo ir akustinės aplinkos. Daugiau informacijos žr. garso lygio diagramose."]
["","","","","","(3) - Garso galios lygis yra absoliuti reikšmė nurodanti galią, kurią sukuria garso šaltinis.","(3) - Garso galios lygis yra absoliuti reikšmė nurodanti galią, kurią sukuria garso šaltinis."]
["Vamzdžių jungtys","Liquid","","OD","mm","","6.35"]
["","Dujos","","Iš. diam.","mm","","9.52"]
["","Drenažo vamzdis","","","","","27.2"]