{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":19,"n_cols":5,"rows_kept":19,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDQ-B / RZQ-BW1"]
[]
[]
[]
[]
["","","","","FDQ125B8V3B9 / RZQ125B8W1B"]
["Vėsinimo pajėgumas","Nom.","","kW","12.50 (1)"]
["Vamzdžių jungtys","Skysčių vamzdis","OD","mm","9.52"]
["","Dujos","Iš. diam.","mm","15.9"]
["","Drenažo vamzdis","OD","mm","26"]
["Vardinis našumas","Metinis energijos sunaudojimas","","kWh","2,075"]
["","EER","","","3.01"]
["","COP","","","3.79"]
["","Energijos suvartojimo ženklinimo direktyva","Vėsinimas","","B"]
["","","Šildymas","","A"]
["Šildymo galingumas","Nom.","","kW","14.00 (2)"]
["Pastabos","","","","(1) - Aušinimas: vidaus temp. 27 °CDB, 19 °CWB; lauko temp. 35 °CDB; ekvivalentinis vamzdyno ilgis: 7,5 m; aukščių skirtumas: 0 m"]
["","","","","(2) - Šildymas: vidaus temp. 20 °CDB; lauko temp. 7 °CDB, 6 °CWB; ekvivalentinis aušinimo medžiagos vamzdyno ilgis: 7,5 m; aukščių skirtumas: 0 m"]
["","","","","(3) - Nominalus efektyvumas: vėsinimas esant 35°/27° nominaliąja apkrova, šildymas esant 7°/20° nominaliąja apkrova"]