{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":23,"n_cols":5,"rows_kept":23,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDQ-C / RZQG-L9V1"]
[]
[]
[]
[]
["","","","","FDQ125C5VEB / RZQG125L9V1B"]
["Aušinimo galingumas","Nom.","","kW","12.0"]
["Erdvės vėsinimas","SEER","","","5.81"]
["","Metinės energijos sąnaudos","","kWh/m.","723"]
["","Vėsinimas","Pdesign","kW","12.00"]
["","Energijos efektyvumo klasė","","","A+"]
["Patalpos šildymas (vidutinis klimatas)","Pajėgumas","Pdesign","kW","12.71"]
["","SCOP/A","","","4.21"]
["","Energijos efektyvumo klasė","","","A+"]
["","Metinės energijos sąnaudos","","kWh/m.","4,227"]
["Vardinis našumas","Metinis energijos sunaudojimas","","kWh","1,600"]
["","EER","","","3.75"]
["","COP","","","3.83"]
["","Energijos suvartojimo ženklinimo direktyva","Vėsinimas","","A"]
["","","Šildymas","","A"]
["Šildymo galingumas","Nom.","","kW","13.5"]
["Pastabos","","","","(1) - EER/COP pagal „Eurovent 2012“, skirta naudoti tik už ES ribų"]
["","","","","(2) - Nominalus efektyvumas: vėsinimas esant 35°/27° nominaliąja apkrova, šildymas esant 7°/20° nominaliąja apkrova"]