{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":28,"n_cols":7,"rows_kept":28,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDQ-C / RZQSG-LV1/LY1"]
[]
[]
[]
[]
["","","","","FDQ125C7VEB / RZQSG125L7V1B","FDQ125C7VEB / RZQSG125L7Y1B9","FDQ125C7VEB / RZQSG125L7Y1B"]
["Aušinimo galingumas","Nom.","","kW","12.0","12.0","12.0 (3)"]
["Patalpos vėsinimas","SEER","","","4.35","4.35","4.35 (6)"]
["","Metinės energijos sąnaudos","","kWh/a","965.517","965.517"]
["","Vėsinimas","Pdesign","kW","12.00","12.00"]
["","Energijos efektyvumo klasė","","","C","C"]
["Patalpos šildymas (vidutinis klimatas)","Pajėgumas","Pdesign","kW","7.60","7.60"]
["","SCOP/A","","","3.81","3.81","3.81 (6)"]
["","Energijos efektyvumo klasė","","","A","A"]
["","Metinės energijos sąnaudos","","kWh/a","2,791","2,791"]
["Vardinis našumas","Metinis energijos sunaudojimas","","kWh","1,870","1,600","1,870"]
["","EER","","","3.21","3.21","3.21"]
["","COP","","","3.51","3.51","3.51"]
["","Energijos suvartojimo ženklinimo direktyva","Vėsinimas","","A","A","A"]
["","","Šildymas","","B","B","B"]
["Šildymo galingumas","Nom.","","kW","13.5","13.5","13.5 (4)"]
["Pastabos","","","","(1) - EER/COP pagal „Eurovent 2012“, skirta naudoti tik už ES ribų","(1) - EER/COP pagal „Eurovent 2012“, skirta naudoti tik už ES ribų","(1) - Energijos suvartojimas per metus: apskaičiuota pagal vidutinį 500 valandų naudojimą per metus esant pilnai apkrovai (nominaliomis sąlygomis)"]
["","","","","(2) - Nominalus efektyvumas: vėsinimas esant 35°/27° nominaliąja apkrova, šildymas esant 7°/20° nominaliąja apkrova","(2) - Nominalus efektyvumas: vėsinimas esant 35°/27° nominaliąja apkrova, šildymas esant 7°/20° nominaliąja apkrova","(2) - Energijos žymuo: skalė nuo A (efektyviausia) iki G (mažiau efektyvu)"]
["","","","","","","(3) - Aušinimas: vidaus temp. 27 °CDB, 19 °CWB; lauko temp. 35 °CDB; ekvivalentinis vamzdyno ilgis: 5 m; aukščių skirtumas: 0 m"]
["","","","","","","(4) - Šildymas: vidaus temp. 20 °CDB; lauko temp. 7 °CDB, 6 °CWB; ekvivalentinis aušinimo medžiagos vamzdyno ilgis: 5 m; aukščių skirtumas: 0 m"]
["","","","","","","(5) - Metinės energijos sąnaudos pagal energijos žymėjimo direktyvą 2002/31/EB"]
["","","","","","","(6) - SEER ir SCOP pagal EN 14825"]
["","","","","","","(7) - Nominalus efektyvumas: vėsinimas esant 35°/27° nominaliąja apkrova, šildymas esant 7°/20° nominaliąja apkrova"]