{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":45,"n_cols":6,"rows_kept":45,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDQ-C"]
[]
[]
[]
[]
["","","","","FDQ125C5VEB","FDQ125C7VEB"]
["Garso slėgio lygis","Šildymas","Aukštas","dBA","40","40"]
["","","Žemas","dBA","33","33"]
["","Aušinimas","Žemas","dBA","33","33"]
["","","Aukštas","dBA","40","40"]
["Kontrolės sistemos","Wired remote control","","","BRC1D52, BRC1E53A, BRC1E53B, BRC1E53C","BRC1D52, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D528"]
["","Nuotolinis valdymas infraraudonaisiais spinduliais","","","BRC4C65","BRC4C65"]
["Aušinimo galingumas","Bendras galingumas","Nom.","kW","12.5 (1)","12.5"]
["Vamzdžių jungtys","Skystis","OD","mm","9.52","9.52"]
["","Dujos","Iš. diam.","mm","15.9","15.9"]
["","Drenažo vamzdis","","","VP25 (I.D. 25/O.D. 32)","VP25 (I.D. 25/O.D. 32)"]
["Tiekiamas galingumas","Aušinimas","Nom.","kW","0.35"]
["","Šildymas","Nom.","kW","0.35"]
["Reikiama anga lubose >","mm","","","350","350"]
["Sound power level","Vėsinimas","","dBA","66","66"]
["Matmenys","Įrenginys","Plotis","mm","1,400","1,400"]
["","","Gylis","mm","700","700"]
["","","Aukštis","mm","300","300"]
["Korpusas","Medžiaga","","","","Galvanizuotas plienas"]
["","Spalva","","","Nedažytas (galvanizuotas)","Not painted"]
["Svoris","Įrenginys","","kg","45","45"]
["Ventiliatorius","Išorinis statinis slėgis","Aukštas","Pa","200","200"]
["","","Nom.","Pa","50","50"]
["Drenavimo aukštis","mm","","","625","625"]
["Dekoratyvinis skydelis","Svoris","","kg","6.5","6.5"]
["","Modelis","","","BYBS125DJW1","BYBS125DJW1"]
["","Matmenys","Aukštis","mm","55","55"]
["","","Gylis","mm","500","500"]
["","","Plotis","mm","1,500","1,500"]
["","Spalva","","","Balta spalva (10Y9/0.5)","Balta spalva (10Y9/0.5)"]
["Šildymo galingumas","Bendras pajėgumas","Nom.","kW","14.0 (2)","14.0"]
["Power supply","Fazė","","","1~","1~"]
["","Dažnis","","Hz","50/60","50/60"]
["","Pavadinimas","","","VE","VE"]
["","Įtampa","","V","220-240/220","220-240/220"]
["Pastabos","","","","(1) - Aušinimas: vidinė temp. 27 °CDB, 19,0 °CWB lauko temp. 35 °CDB; ekvivalentinis vamzdyno ilgis: 7,5 m; lygių skirtumas: 0 m","(1) - Šildymas: vidaus temp. 20 °CDB; lauko temp. 7 °CDB, 6 °CWB; ekvivalentinis aušinimo medžiagos vamzdyno ilgis: 7,5 m; aukščių skirtumas: 0 m"]
["","","","","(2) - Šildymas: vidaus temp. 20 °CDB; lauko temp. 7 °CDB, 6 °CWB; ekvivalentinis aušinimo medžiagos vamzdyno ilgis: 7,5 m; aukščių skirtumas: 0 m","(2) - Aušinimo galia yra bendra galia, įskaitant vidaus patalpų ventiliatoriaus kaitimo aušinimo (priedą prie šildymo) mažinimą."]
["","","","","(3) - Aušinimo galia yra bendra galia, įskaitant vidaus patalpų ventiliatoriaus kaitimo aušinimo (priedą prie šildymo) mažinimą.","(3) - Garso slėgio reikšmės nurodomos įrenginiui, kuris sumontuotas su siurbimu gale."]
["","","","","(4) - Garso slėgio reikšmės nurodomos įrenginiui, kuris sumontuotas su siurbimu gale.","(4) - PED įrenginio kategorija: neįtraukiama į PED sritį dėl 97/23/EB 1 straipsnio 3.6 pastraipos"]
["","","","","(5) - PED įrenginio kategorija: neįtraukiama į PED sritį dėl 97/23/EB 1 straipsnio 3.6 pastraipos","(5) - Aušinimas: vidaus temp. 27 °CDB, 19 °CWB; lauko temp. 35 °CDB; ekvivalentinis vamzdyno ilgis: 7,5 m (horizontaliai); aukščių skirtumas: 0 m"]