{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":15,"n_cols":6,"rows_kept":15,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDXM-F3 / 2MXM-M"]
[]
[]
[]
[]
["","","","","FDXM25F3V1B / FDXM25F3V1B / 2MXM40M3V1B","FDXM25F3V1B / FDXM35F3V1B / 2MXM40M3V1B"]
["Vėsinimo pajėgumas","Nom.","","kW","4.0","4.0"]
["Vardinis našumas","Metinis energijos sunaudojimas","","kWh","563","555"]
["","EER","","","3.55","3.60"]
["","COP","","","4.13","4.17"]
["","Energijos suvartojimo ženklinimo direktyva","Vėsinimas","","A","A"]
["","","Šildymas","","A","A"]
["Šildymo galingumas","Nom.","","kW","4.20","4.20"]
["Pastabos","","","","(1) - Nom. vėsinimas pagrįstas: vidaus temp.: 27 °CDB, 19 °CWB, lauko temp.: 35 °CDB, ekviv. šaltnešio vamzdynas: 5 m., lygių skirtumas: 0 m. Standartinio efektyvumo serijos duomenys","(1) - Nom. vėsinimas pagrįstas: vidaus temp.: 27 °CDB, 19 °CWB, lauko temp.: 35 °CDB, ekviv. šaltnešio vamzdynas: 5 m., lygių skirtumas: 0 m. Standartinio efektyvumo serijos duomenys"]
["","","","","(2) - Nominali šildymo galia nustatyta remiantis: vidaus temperatūra: 20 °CDB, lauko temperatūra: 7 °CDB, 6 °CWB, ekvivalentinis aušinimo medžiagos vamzdyno ilgis: 5 m, aukščių skirtumas: 0 m.","(2) - Nominali šildymo galia nustatyta remiantis: vidaus temperatūra: 20 °CDB, lauko temperatūra: 7 °CDB, 6 °CWB, ekvivalentinis aušinimo medžiagos vamzdyno ilgis: 5 m, aukščių skirtumas: 0 m."]