{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":39,"n_cols":8,"rows_kept":39,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDXM-F3"]
[]
[]
[]
[]
["","","","","FDXM25F3V1B","FDXM35F3V1B","FDXM50F3V1B","FDXM60F3V1B"]
["Garso slėgio lygis","Šildymas","Aukštas","dBA","35","35","38","38"]
["","","Vidutinis","dBA","33","33","35","35"]
["","","Žemas","dBA","27","27","30","30"]
["","Aušinimas","Vidutinis","dBA","33","33","35","35"]
["","","Žemas","dBA","27","27","30","30"]
["","","Aukštas","dBA","35","35","38","38"]
["Standartiniai priedai","Įrengimo vadovas","","","1","1","1","1"]
["","Eksploatavimo vadovas","","","1","1","1","1"]
["","Izoliacija priedui","","","1","1","1","1"]
["","Sandarinimo tarpiklis","","","1","1","1","1"]
["","Metalinis veržtuvas","","","1","1","1","1"]
["","Drenavimo žarna","","","1","1","1","1"]
["","Poveržlė kablio laikytuvui","","","8","8","8","8"]
["","Sandarinimo medžiaga","","","2","2","2","2"]
["","Veržtuvai","","","6","6","6","6"]
["","Poveržlę fiksuojanti plokštė","","","4","4","4","4"]
["","Varžtai vamzdžių antbriauniams","","","1","1","1","1"]
["","Oro filtras","","","1","1","1","1"]
["Vamzdžių jungtys","Skystis","OD","mm","6.35","6.35","6.35","6.35"]
["","Dujos","Iš. diam.","mm","9.50","9.50","12.70","12.70"]
["","Drenažo vamzdis","","","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)"]
["Power input","Aušinimas","Nom.","kW","0.036","0.036","0.060","0.060"]
["","Šildymas","Nom.","kW","0.036","0.036","0.060","0.060"]
["Sound power level","Vėsinimas","","dBA","53","53","55","56"]
["","Šildymas","","dBA","53","53","55","56"]
["Matmenys","Įrenginys","Plotis","mm","750","750","1,150","1,150"]
["","","Gylis","mm","620","620","620","620"]
["","","Aukštis","mm","200","200","200","200"]
["Svoris","Įrenginys","","kg","21","21","28","28"]
["Ventiliatorius","Išorinis statinis slėgis","Nom.","Pa","30","30","40","40"]
["Power supply","Fazė","","","1~","1~","1~","1~"]
["","Dažnis","","Hz","50","50","50","50"]
["","Įtampa","","V","220-240","220-240","220-240","220-240"]