{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":30,"n_cols":6,"rows_kept":30,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDXM-F9 / RXM-A"]
[]
[]
[]
[]
["","","","","FDXM50F3V1B9 / RXM50A5V1B","FDXM60F3V1B9 / RXM60A5V1B"]
["Aušinimo galingumas","Min.","","kW","1.70","1.7"]
["","Nom.","","kW","5.00","6"]
["","Maks.","","kW","5.30","6.5"]
["Šildymo galingumas","Min.","","kW","1.70","1.7"]
["","Nom.","","kW","5.80","7"]
["","Maks.","","kW","6.00","7.1"]
["Nominalus efektyvumas","EER","","","3.06","2.93"]
["","COP","","","3.10","3.21"]
["","Metinis energijos sunaudojimas","","kWh","817","1024"]
["Vardinis našumas","Energijos suvartojimo ženklinimo direktyva","Vėsinimas","","B","C"]
["","","Šildymas","","D","C"]
["Patalpos vėsinimas","Energijos efektyvumo klasė","","","A+","A"]
["","Vėsinimas","Pdesign","kW","5.00","6"]
["","SEER","","","5.77","5.56"]
["","Metinės energijos sąnaudos","","kWh/a","303","378"]
["Patalpos šildymas (vidutinis klimatas)","Energijos efektyvumo klasė","","","A","A"]
["","Pajėgumas","Pdesign","kW","4.00","4.6"]
["","SCOP/A","","","3.93","3.8"]
["","Pdh Šildymo pajėgumas esant –10°","","kW","3.54","3.94"]
["","Metinės energijos sąnaudos","","kWh/a","1424","1693"]
["Pastabos","","","","","(1) - Nominalus aušinimo galingumas yra pagrįstas: patalpų temp.: 27°CDB/19°CWB, išorinė temperatūra: 35 °CDB, ekvivalentinis šaltnešio vamzdynas: 5 m, aukščio skirtumas: 0 m."]
["","","","","","(2) - Nominali šildymo galia nustatyta remiantis: vidaus temperatūra: 20 °CDB, lauko temperatūra: 7 °CDB, 6 °CWB, ekvivalentinis aušinimo medžiagos vamzdyno ilgis: 5 m, aukščių skirtumas: 0 m."]
["","","","","","(3) - Žr. specialų darbinio diapazono brėžinį"]
["","","","","","(4) - Žr. atskirą elektros duomenų brėžinį"]