{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":25,"n_cols":9,"rows_kept":25,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDXM-F9 / RZAG-A"]
[]
[]
[]
[]
["","","","","FDXM35F3V1B9 / RZAG35A2V1B","FDXM50F3V1B9 / RZAG35A2V1B","FDXM50F3V1B9 / RZAG50A2V1B","FDXM60F3V1B9 / RZAG50A2V1B","FDXM60F3V1B9 / RZAG60A2V1B"]
["Aušinimo galingumas","Min.","","kW","1.6","1.6","1.7","1.7","1.7"]
["","Maks.","","kW","4.5","4.5","6.0","6.0","6.5"]
["","Nom.","","kW","3.5","3.5","5.0","5.0","6.0"]
["Erdvės vėsinimas","SEER","","","5.90","6.08","5.90","5.98","5.70"]
["","Metinės energijos sąnaudos","","kWh/a","208","201","296","293","368"]
["","Vėsinimas","Pdesign","kW","3.50","3.50","5.00","5.00","6.00"]
["","Energijos efektyvumo klasė","","","A+","A+","A+","A+","A+"]
["Patalpos šildymas (vidutinis klimatas)","Pajėgumas","Pdesign","kW","3.50","4.20","4.30","4.30","4.50"]
["","SCOP/A","","","3.90","4.05","3.90","3.94","3.90"]
["","Energijos efektyvumo klasė","","","A","A+","A","A","A"]
["","Metinės energijos sąnaudos","","kWh/a","1,255","1,451","1,544","1,526","1,616"]
["Vardinis našumas","Metinis energijos sunaudojimas","","kWh","449","432","658","628","882"]
["","EER","","","3.90","4.05","3.80","3.98","3.40"]
["","COP","","","3.50","3.63","3.40","3.44","3.30"]
["","Energijos suvartojimo ženklinimo direktyva","Vėsinimas","","A","A","A","A","A"]
["","","Šildymas","","B","A","C","B","C"]
["Šildymo galingumas","Nom.","","kW","4.00","4.00","5.00","5.00","7.00"]
["","Min.","","kW","1.40","1.40","1.70","1.70","1.70"]
["","Maks.","","kW","5.00","5.00","6.00","6.00","7.50"]