{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":27,"n_cols":9,"rows_kept":27,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDXM-F9 / RZAG-B"]
[]
[]
[]
[]
["","","","","FDXM50F3V1B9 / RZAG35B5V1B","FDXM35F3V1B9 / RZAG35B5V1B","FDXM60F3V1B9 / RZAG50B5V1B","FDXM50F3V1B9 / RZAG50B5V1B","FDXM60F3V1B9 / RZAG60B5V1B"]
["Aušinimo galingumas","Min.","","kW","1.6","1.6","1.7","1.7","1.7"]
["","Nom.","","kW","3.5","3.5","5","5","6"]
["","Maks.","","kW","4.5","4.5","6","6","6.5"]
["Šildymo galingumas","Min.","","kW","1.4","1.4","1.7","1.7","1.7"]
["","Nom.","","kW","4","4","5","5","7"]
["","Maks.","","kW","5","5","6","6","7.5"]
["Nominalus efektyvumas","EER","","","4.05","3.9","3.98","3.8","3.4"]
["","COP","","","3.63","3.5","3.44","3.4","3.3"]
["","Metinis energijos sunaudojimas","","kWh","432","449","628","658","882"]
["Vardinis našumas","Energijos suvartojimo ženklinimo direktyva","Vėsinimas","","A","A","A","A","A"]
["","","Šildymas","","A","B","B","C","C"]
["Patalpos vėsinimas","Energijos efektyvumo klasė","","","A+","A+","A+","A+","A+"]
["","Vėsinimas","Pdesign","kW","3.5","3.5","5","5","6"]
["","SEER","","","6.08","5.9","5.98","5.9","5.7"]
["","Metinės energijos sąnaudos","","kWh/a","201","208","293","296","368"]
["Patalpos šildymas (vidutinis klimatas)","Energijos efektyvumo klasė","","","A+","A","A","A","A"]
["","Pajėgumas","Pdesign","kW","4.2","3.5","4.3","4.3","4.5"]
["","SCOP/A","","","4.05","3.9","3.94","3.9","3.9"]
["","Pdh Šildymo pajėgumas esant –10°","","kW","3.49","2.99","3.63","3.62","3.82"]
["","Metinės energijos sąnaudos","","kWh/a","1451","1255","1526","1544","1616"]
["Energijos naudojimo efektyvumo klasė","","","","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D"]