{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":85,"n_cols":9,"rows_kept":85,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDXM-F9"]
[]
[]
[]
[]
["","","","","","FDXM25F3V1B9","FDXM35F3V1B9","FDXM50F3V1B9","FDXM60F3V1B9"]
["Garso slėgio lygis","Šildymas","","Aukštas","dBA","35.0","35.0","","38.0"]
["","","","Vidutinis","dBA","33.0","33.0","","35.0"]
["","","","Žemas","dBA","27.0","27.0","","30.0"]
["","Aušinimas","","Vidutinis","dBA","33.0","33.0","","35.0"]
["","","","Žemas","dBA","27.0","27.0","","30.0"]
["","","","Aukštas","dBA","35.0","35.0","","38.0"]
["Standartiniai priedai","Įrengimo vadovas","","","","1","1","","1"]
["","Eksploatavimo vadovas","","","","1","1","","1"]
["","Izoliacija priedui","","","","1","1","","1"]
["","Sandarinimo tarpiklis","","","","1","1","","1"]
["","Metalinis veržtuvas","","","","1","1","","1"]
["","Drenavimo žarna","","","","1","1","","1"]
["","Poveržlė kablio laikytuvui","","","","8","8","","8"]
["","Sandarinimo medžiaga","","","","2","2","","2"]
["","Veržtuvai","","","","6","6","","6"]
["","Poveržlę fiksuojanti plokštė","","","","4","4","","4"]
["","Varžtai vamzdžių antbriauniams","","","","1","1","","1"]
["","Oro filtras","","","","1","1","","1"]
["Vamzdžių jungtys","Skystis","","OD","mm","6.35","6.35","","6.35"]
["","Dujos","","Iš. diam.","mm","9.50","9.50","","12.70"]
["","Drain","","","","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","","VP20 (I.D. 20/O.D. 26)"]
["Tiekiama galia","Aušinimas","","Nom.","kW","0.036","0.036","","0.060"]
["","Šildymas","","Nom.","kW","0.036","0.036","","0.060"]
["Sound power level","Vėsinimas","","","dBA","53.0","53.0","","56.0"]
["","Šildymas","","","dBA","53.0","53.0","","56.0"]
["Matmenys","Įrenginys","","Plotis","mm","750","750","","1,150"]
["","","","Gylis","mm","620","620","","620"]
["","","","Aukštis","mm","200","200","","200"]
["Svoris","Įrenginys","","","kg","21","21","","28"]
["Ventiliatorius","Išorinis statinis slėgis","","Nom.","Pa","30","30","","40"]
["","Oro debitas","Šildymas","Didelis","m³/min.","8.7","8.7","","16.0"]
["","","","Vidutinis","m³/min.","8.0","8.0","","14.8"]
["","","","Mažas","m³/min.","7.3","7.3","","13.5"]
["","","Aušinimas","Mažas","m³/min.","7.3","7.3","","13.5"]
["","","","Vidutinis","m³/min.","8.0","8.0","","14.8"]
["","","","Didelis","m³/min.","8.7","8.7","","16.0"]
["Power supply","Fazė","","","","1~","1~","","1~"]
["","Dažnis","","","Hz","50","50","","50"]
["","Voltage","","","V","220-240","220-240","","220-240"]
["Pastabos","","","","","(1) - Žr. atskirą elektros duomenų brėžinį","(1) - Žr. atskirą elektros duomenų brėžinį","","(1) - Žr. atskirą elektros duomenų brėžinį"]
["Tiekiama galia","Aušinimas","","Nom.","kW","","","0.060"]
["","Šildymas","","Nom.","kW","","","0.060"]
["Matmenys","Įrenginys","","Aukštis","mm","","","200"]
["","","","Plotis","mm","","","1150"]
["","","","Gylis","mm","","","620"]
["Svoris","Įrenginys","","","kg","","","28"]
["Ventiliatorius","Oro debitas","Aušinimas","Didelis","m³/min.","","","15.8"]
["","Oro srauto greitis","Vėsinimas","Vidutinis","m³/min.","","","14.6"]
["","","","Mažas","m³/min.","","","13.3"]
["","","Šildymas","Didelis","m³/min.","","","15.8"]
["","Oro srauto greitis","Šildymas","Vidutinis","m³/min.","","","14.6"]
["","","Šildymas","Mažas","m³/min.","","","13.3"]
["","Išorinis statinis slėgis","","Nom.","Pa","","","40"]
["Garso galingumo lygis","Vėsinimas","","","dBA","","","55.0"]
["","Šildymas","","","dBA","","","55.0"]
["Garso slėgio lygis","Aušinimas","","Aukštas","dBA","","","38.0"]
["","Vėsinimas","","Vidutinis","dBA","","","35.0"]
["","","","Žemas","dBA","","","30.0"]
["","Šildymas","","Aukštas","dBA","","","38.0"]
["","","","Vidutinis","dBA","","","35.0"]
["","","","Žemas","dBA","","","30.0"]
["Vamzdžių jungtys","Skystis","","OD","mm","","","6.35"]
["","Dujos","","Iš. diam.","mm","","","12.70"]
["","Drenažas","","","","","","VP20 (I.D. 20/O.D. 26)"]
["Standartiniai priedai","Installation manual","","","","","","1"]
["","Washer for hanger bracket","","","","","","8"]
["","Operation manual","","","","","","1"]
["","Clamp metal","","","","","","1"]
["","Clamps","","","","","","6"]
["","Drain hose","","","","","","1"]
["","Oro filtras","","","","","","1"]
["","Insulation for fitting","","","","","","1"]
["","Screws for duct flanges","","","","","","1"]
["","Sealing material","","","","","","2"]
["","Sealing pad","","","","","","1"]
["","Washer fixing plate","","","","","","4"]
["El. tiekimas","Fazė","","","","","","1~"]
["Maitinimas","Dažnis","","","Hz","","","50"]
["","Įtampa","","","V","","","220-240"]