{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":41,"n_cols":5,"rows_kept":41,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDXS-F9"]
[]
[]
[]
[]
["","","","","FDXS50F2VEB9"]
["Garso slėgio lygis","Šildymas","Aukštas","dBA","38"]
["","","Vidutinis","dBA","36"]
["","","Žemas","dBA","30"]
["","Aušinimas","Vidutinis","dBA","36"]
["","","Žemas","dBA","30"]
["","","Aukštas","dBA","38"]
["Standartiniai priedai","Įrengimo vadovas","","","1"]
["","Eksploatavimo vadovas","","","1"]
["","Izoliacija priedui","","","1"]
["","Sandarinimo tarpiklis","","","1"]
["","Metalinis veržtuvas","","","1"]
["","Drenavimo žarna","","","1"]
["","Poveržlė kablio laikytuvui","","","8"]
["","Sandarinimo medžiaga","","","2"]
["","Veržtuvai","","","6"]
["","Poveržlę fiksuojanti plokštė","","","4"]
["","Varžtai vamzdžių antbriauniams","","","1"]
["","Oro filtras","","","1"]
["Vamzdžių jungtys","Skystis","OD","mm","6.35"]
["","Dujos","Iš. diam.","mm","12.7"]
["","Drenažo vamzdis","","","VP20 (I.D. 20/O.D. 26)"]
["Power input","Aušinimas","Nom.","kW","0.060"]
["","Šildymas","Nom.","kW","0.060"]
["Sound power level","Vėsinimas","","dBA","55"]
["","Šildymas","","dBA","55"]
["Matmenys","Įrenginys","Plotis","mm","1,150"]
["","","Gylis","mm","620"]
["","","Aukštis","mm","200"]
["Svoris","Įrenginys","","kg","30.0"]
["Ventiliatorius","Išorinis statinis slėgis","Nom.","Pa","40"]
["Power supply","Fazė","","","1~"]
["","Dažnis","","Hz","50/60"]
["","Pavadinimas","","","VE"]
["","Įtampa","","V","220-240"]
["Pastabos","","","","(1) - Kai sujungtas su sudėtinės sistemos išoriniu įrenginiu, žr. sudėtinio išorinio įrenginio specifikacijas prie kurios jungsite."]