{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":18,"n_cols":11,"rows_kept":18,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FFA-A / RZQG-L(8)Y1"]
[]
[]
[]
[]
["","","","","FFA35A2VEB / FFA35A2VEB / FFA35A2VEB / FFA35A2VEB / RZQG125L8Y1B","FFA35A2VEB / FFA35A2VEB / FFA35A2VEB / RZQG100L8Y1B","FFA50A2VEB / FFA50A2VEB / FFA50A2VEB / RZQG125L8Y1B","FFA50A2VEB / FFA50A2VEB / RZQG100L8Y1B","FFA60A2VEB / FFA60A2VEB / RZQG125L8Y1B","FFA35A2VEB / FFA35A2VEB / RZQG71L8Y1B","FFA50A2VEB / FFA50A2VEB / RZQG71L8Y1B"]
["Energijos naudojimo efektyvumo klasė","","","","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D"]
["Patalpos vėsinimas","SEER","","","","","","","","5.10","5.10"]
["","Metinės energijos sąnaudos","","kWh/a","","","","","","467","467"]
["","Vėsinimas","Pdesign","kW","","","","","","6.80","6.80"]
["","Energijos efektyvumo klasė","","","","","","","","A","A"]
["Patalpos šildymas (vidutinis klimatas)","Pajėgumas","Pdesign","kW","","","","","","6.00","6.00"]
["","SCOP/A","","","","","","","","3.80","3.80"]
["","Energijos efektyvumo klasė","","","","","","","","A","A"]
["","Metinės energijos sąnaudos","","kWh/a","","","","","","2,211","2,211"]
["Pastabos","","","","","","","","","(1) - Aušinimas: vidaus temp. 27 °CDB, 19 °CWB; lauko temp. 35 °CDB; ekvivalentinis vamzdyno ilgis: 7,5 m; aukščių skirtumas: 0 m"]
["","","","","","","","","","(2) - Šildymas: vidaus temp. 20 °CDB; lauko temp. 7 °CDB, 6 °CWB; ekvivalentinis aušinimo medžiagos vamzdyno ilgis: 7,5 m; aukščių skirtumas: 0 m"]
["","","","","","","","","","(3) - EER/COP pagal „Eurovent 2012“, skirta naudoti tik už ES ribų"]