{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":43,"n_cols":10,"rows_kept":43,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FFA-A9 / RXM-N9"]
[]
[]
[]
[]
["","","","","FFA25A2VEB9 / RXM25N2V1B9","FFA25A2VEB9 / RXM25N5V1B9","FFA35A2VEB9 / RXM35N2V1B9","FFA35A2VEB9 / RXM35N5V1B9","FFA50A2VEB9 / RXM50N2V1B9","FFA60A2VEB9 / RXM60N2V1B9"]
["Aušinimo galingumas","Nom.","","kW","2.50","2.50"]
["Erdvės vėsinimas","SEER","","","6.17","6.17"]
["","Metinės energijos sąnaudos","","kWh/a","142","142"]
["","Vėsinimas","Pdesign","kW","2.50","2.50"]
["","Energijos efektyvumo klasė","","","A++","A++"]
["Patalpos šildymas (vidutinis klimatas)","Pajėgumas","Pdesign","kW","2.31","2.31"]
["","SCOP/A","","","4.24","4.24"]
["","Energijos efektyvumo klasė","","","A+","A+"]
["","Metinės energijos sąnaudos","","kWh/a","762","762"]
["Vardinis našumas","Metinis energijos sunaudojimas","","kWh","273","273"]
["","EER","","","4.57","4.57"]
["","COP","","","3.90","3.90"]
["","Energijos suvartojimo ženklinimo direktyva","Vėsinimas","","A","A"]
["","","Šildymas","","A","A"]
["Šildymo galingumas","Nom.","","kW","3.20","3.20"]
["Pastabos","","","","(1) - Žr. atskirą elektros duomenų brėžinį","(1) - Žr. atskirą elektros duomenų brėžinį"]
["","","","","(2) - Žr. specialų darbinio diapazono brėžinį","(2) - Žr. specialų darbinio diapazono brėžinį"]
["","","","","(3) - Nominalus aušinimo galingumas yra pagrįstas: patalpų temp.: 27°CDB/19°CWB, išorinė temperatūra: 35 °CDB, ekvivalentinis šaltnešio vamzdynas: 5 m, aukščio skirtumas: 0 m.","(3) - Nominalus aušinimo galingumas yra pagrįstas: patalpų temperatūra: 27°CDB/19°CWB, išorinė temperatūra: 35 °CDB, ekvivalentinis šaltnešio vamzdynas: 5 m, aukščio skirtumas: 0 m."]
["","","","","(4) - Nominali šildymo galia nustatyta remiantis: vidaus temperatūra: 20 °CDB, lauko temperatūra: 7 °CDB, 6 °CWB, ekvivalentinis aušinimo medžiagos vamzdyno ilgis: 5 m, aukščių skirtumas: 0 m.","(4) - Nominali šildymo galia nustatyta remiantis: vidaus temperatūra: 20 °CDB, lauko temperatūra: 7 °CDB, 6 °CWB, ekvivalentinis aušinimo medžiagos vamzdyno ilgis: 5 m, aukščių skirtumas: 0 m."]
["Outdoor unit","","","","","","RXM35N2V1B9","RXM35N5V1B9","","RXM60N2V1B9"]
["Aušinimo galingumas","Nom.","","kW","","","3.40","3.40","5.00","5.70"]
["Šildymo galingumas","Nom.","","kW","","","4.20","4.20","5.80","7.00"]
["Nominalus efektyvumas","EER","","","","","3.81","3.81","3.24","3.05"]
["","COP","","","","","3.50","3.50","3.49","3.41"]
["","Metinis energijos sunaudojimas","","kWh","","","446","446","772","934"]
["Vardinis našumas","Energijos suvartojimo ženklinimo direktyva","Vėsinimas","","","","A","A","A","B"]
["","","Šildymas","","","","B","B","B","B"]
["Patalpos vėsinimas","Energijos efektyvumo klasė","","","","","A++","A++","A+","A+"]
["","Vėsinimas","Pdesign","kW","","","3.40","3.40","5.00","5.70"]
["","SEER","","","","","6.38","6.38","5.98","5.76"]
["","Metinės energijos sąnaudos","","kWh/a","","","186","186","293","347"]
["Patalpos šildymas (vidutinis klimatas)","Energijos efektyvumo klasė","","","","","A+","A+","A","A+"]
["","Pajėgumas","Pdesign","kW","","","3.10","3.10","3.84","3.96"]
["","SCOP/A","","","","","4.10","4.10","3.90","4.04"]
["","Pdh Šildymo pajėgumas esant –10°","","kW","","","2.04","2.04","3.40","3.66"]
["","Metinės energijos sąnaudos","","kWh/a","","","1058","1058","1378","1372"]
["Energijos naudojimo efektyvumo klasė","","","","","","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D"]