{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":64,"n_cols":8,"rows_kept":64,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FFA-A9"]
[]
[]
[]
[]
["","","","","","FFA25A2VEB9","FFA35A2VEB9","FFA60A2VEB9"]
["Korpusas","Medžiaga","","","","Galvanizuoto plieno plokštė","Galvanizuoto plieno plokštė","Galvanizuoto plieno plokštė"]
["Matmenys","Įrenginys","","Aukštis","mm","260","260","260"]
["","","","Plotis","mm","575","575","575"]
["","","","Gylis","mm","575","575","575"]
["Svoris","Įrenginys","","","kg","16.0","16.0","17.5"]
["Ventiliatorius","Oro debitas","Aušinimas","Didelis","m³/min.","9.0","10.0","14.5"]
["","Oro srauto greitis","Vėsinimas","Vidutinis","m³/min.","8.0","8.5","12.5"]
["","","","Mažas","m³/min.","6.5","6.5","9.5"]
["","","Šildymas","Didelis","m³/min.","9.0","10.0","14.5"]
["","Oro srauto greitis","Šildymas","Vidutinis","m³/min.","8.0","8.5","12.5"]
["","","Šildymas","Mažas","m³/min.","6.5","6.5","9.5"]
["Garso galingumo lygis","Vėsinimas","","","dBA","48.0","51.0","60.0"]
["Garso slėgio lygis","Aušinimas","","Aukštas","dBA","31.0","34.0","43.0"]
["","Vėsinimas","","Vidutinis","dBA","28.5","30.5","40.0"]
["","","","Žemas","dBA","25.0","25.0","32.0"]
["","Šildymas","","Aukštas","dBA","31.0","34.0","43.0"]
["","","","Vidutinis","dBA","28.5","30.5","40.0"]
["","","","Žemas","dBA","25.0","25.0","32.0"]
["Vamzdžių jungtys","Skystis","","OD","mm","6","6","6"]
["","Dujos","","Iš. diam.","mm","9.52","9.52","12.70"]
["","Drenažas","","","","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)"]
["Dekoratyvinis skydelis","Modelis","","","","BYFQ60C2W1W","BYFQ60C2W1W","BYFQ60C2W1W"]
["","Spalva","","","","Balta (N9.5)","Balta (N9.5)","Balta (N9.5)"]
["","Matmenys","","Aukštis","mm","46","46","46"]
["","","","Plotis","mm","620","620","620"]
["","","","Gylis","mm","620","620","620"]
["","Svoris","","","kg","2.8","2.8","2.8"]
["2 dekoratyvinis skydelis","Modelis","","","","BYFQ60C2W1S","BYFQ60C2W1S","BYFQ60C2W1S"]
["","Spalva","","","","Sidabrinė spalva","Sidabrinė spalva","Sidabrinė spalva"]
["","Matmenys","","Aukštis","mm","46","46","46"]
["","","","Plotis","mm","620","620","620"]
["","","","Gylis","mm","620","620","620"]
["","Svoris","","","kg","2.8","2.8","2.8"]
["3 dekoratyvinis skydelis","Modelis","","","","BYFQ60B2W1","BYFQ60B2W1","BYFQ60B2W1"]
["","Spalva","","","","Balta (RAL9010)","Balta (RAL9010)","Balta (RAL9010)"]
["","Matmenys","","Aukštis","mm","55","55","55"]
["","","","Plotis","mm","700","700","700"]
["","","","Gylis","mm","700","700","700"]
["","Svoris","","","kg","2.7","2.7","2.7"]
["4 dekoratyvinis skydelis","Modelis","","","","BYFQ60B3W1","BYFQ60B3W1","BYFQ60B3W1"]
["","Spalva","","","","Balta (RAL9010)","Balta (RAL9010)","Balta (RAL9010)"]
["","Matmenys","","Aukštis","mm","55","55","55"]
["","","","Plotis","mm","700","700","700"]
["","","","Gylis","mm","700","700","700"]
["","Svoris","","","kg","2.7","2.7","2.7"]
["Valdymo sistemos","Nuotolinis infraraudonųjų spindulių pultelis","","","","BRC7EB530 (stand. skydelis), BRC7F530W (baltas skydelis), BRC7F530S (pilkas skydelis)","BRC7EB530 (stand. skydelis), BRC7F530W (baltas skydelis), BRC7F530S (pilkas skydelis)","BRC7EB530 (stand. skydelis), BRC7F530W (baltas skydelis), BRC7F530S (pilkas skydelis)"]
["","Laidinis nuotolinio valdymo pultelis","","","","BRC1D528, BRC1E53A7, BRC1E53B7, BRC1E53C7","BRC1D528, BRC1E53A7, BRC1E53B7, BRC1E53C7","BRC1D528, BRC1E53A7, BRC1E53B7, BRC1E53C7"]
["Standartiniai priedai","Washer for hanger bracket","","","","8","8","8"]
["","Thermal insulation tube","","","","2","2","2"]
["","Hose band","","","","1","1","1"]
["","Drain hose","","","","1","1","1"]
["","Installation and operation manual","","","","1","1","1"]
["","Screws","","","","4","4","4"]
["","Sealing material","","","","4","4","4"]
["","Tie-wraps","","","","7","7","7"]
["El. tiekimas","Fazė","","","","1~","1~","1~"]
["Maitinimas","Dažnis","","","Hz","50","50","50"]
["","Įtampa","","","V","220-240","220-240","220-240"]