{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":16,"n_cols":6,"rows_kept":16,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FHA-A / RR-BW1"]
[]
[]
[]
[]
["","","","","FHA71AVEB / RR71B8W1B","FHA100AVEB / RR100B8W1B"]
["Aušinimo galingumas","Nom.","","kW","7.10 (1)","9.80 (1)"]
["Vamzdžių jungtys","Skystis","OD","mm","9.52","9.52"]
["","Dujos","Iš. diam.","mm","15.9","15.9"]
["","Drenažo vamzdis","OD","mm","26","26"]
["Vardinis našumas","EER","","","2.68","2.66"]
["","Metinis energijos sunaudojimas","","kWh","1,325","1,840"]
["","Energijos suvartojimo ženklinimo direktyva","Vėsinimas","","D","D"]
["Pastabos","","","","(1) - Aušinimas: vidaus temp. 27 °CDB, 19 °CWB; lauko temp. 35 °CDB; ekvivalentinis vamzdyno ilgis: 7,5 m; aukščių skirtumas: 0 m","(1) - Aušinimas: vidaus temp. 27 °CDB, 19 °CWB; lauko temp. 35 °CDB; ekvivalentinis vamzdyno ilgis: 7,5 m; aukščių skirtumas: 0 m"]
["","","","","(2) - Aušinimas: vidaus temp. 27 °CDB, 19 °CWB; lauko temp. 35 °CDB; ekvivalentinis vamzdyno ilgis: 7,5 m (horizontaliai); aukščių skirtumas: 0 m","(2) - Aušinimas: vidaus temp. 27 °CDB, 19 °CWB; lauko temp. 35 °CDB; ekvivalentinis vamzdyno ilgis: 7,5 m (horizontaliai); aukščių skirtumas: 0 m"]
["","","","","(3) - Šildymas: vidaus temp. 20 °CDB; lauko temp. 7 °CDB, 6 °CWB; ekvivalentinis aušinimo medžiagos vamzdyno ilgis: 7,5 m; aukščių skirtumas: 0 m","(3) - Šildymas: vidaus temp. 20 °CDB; lauko temp. 7 °CDB, 6 °CWB; ekvivalentinis aušinimo medžiagos vamzdyno ilgis: 7,5 m; aukščių skirtumas: 0 m"]