{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":28,"n_cols":11,"rows_kept":28,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FHQ-CB"]
[]
[]
[]
[]
["","","","","FHQ35CBVEB","FHQ50CBVEB","FHQ60CBVEB","FHQ71CBVEB","FHQ100CBVEB","FHQ125CBVEB","FHQ140CBVEB"]
["Garso slėgio lygis","Šildymas","Aukštas","dBA","36","37","37","38","42","44","46"]
["","","Nom.","dBA","34","35","35","36","38","41","42"]
["","","Žemas","dBA","31","32","33","34","34","37","38"]
["","Aušinimas","Žemas","dBA","31","32","33","34","34","37","38"]
["","","Aukštas","dBA","36","37","37","38","42","44","46"]
["","","Nom.","dBA","34","35","35","36","38","41","42"]
["Valdymo sistemos","Laidinis nuotolinio valdymo pultelis","","","BRC1D52, BRC1E52A/B, BRC1E53A, BRC1E53B, BRC1E53C, BRC1E51A","BRC1D52, BRC1E52A/B, BRC1E53A, BRC1E53B, BRC1E53C, BRC1E51A","BRC1D52, BRC1E52A/B, BRC1E53A, BRC1E53B, BRC1E53C, BRC1E51A","BRC1D52, BRC1E52A/B, BRC1E53A, BRC1E53B, BRC1E53C, BRC1E51A","BRC1D52, BRC1E52A/B, BRC1E53A, BRC1E53B, BRC1E53C, BRC1E51A","BRC1D52, BRC1E52A/B, BRC1E53A, BRC1E53B, BRC1E53C, BRC1E51A","BRC1D52, BRC1E52A/B, BRC1E53A, BRC1E53B, BRC1E53C, BRC1E51A"]
["","Infrared remote control","","","BRC7G53","BRC7G53","BRC7G53","BRC7G53","BRC7G53","BRC7G53","BRC7G53"]
["Vamzdžių jungtys","Skystis","OD","mm","6.35","6.35","6.35","9.52","9.52","9.52","9.52"]
["","Dujos","Iš. diam.","mm","9.5","12.7","12.7","15.9","15.9","15.9","15.9"]
["","Drenažo vamzdis","","","VP20","VP20","VP20","VP20","VP20","VP20","VP20"]
["Sound power level","Vėsinimas","","dBA","53","54","54","55","60","62","64"]
["","Šildymas","","dBA","53","54","54","55","60","62","64"]
["Matmenys","Įrenginys","Plotis","mm","960","960","1,270","1,270","1,590","1,590","1,590"]
["","","Gylis","mm","690","690","690","690","690","690","690"]
["","","Aukštis","mm","235","235","235","235","235","235","235"]
["Korpusas","Medžiaga","","","Derva, lakštinis metalas","Derva, lakštinis metalas","Derva, lakštinis metalas","Derva, lakštinis metalas","Derva, lakštinis metalas","Derva, lakštinis metalas","Derva, lakštinis metalas"]
["","Spalva","","","Balta spalva","Balta spalva","Balta spalva","Balta spalva","Balta spalva","Balta spalva","Balta spalva"]
["Svoris","Įrenginys","","kg","24","25","31","32","38","38","38"]
["Power supply","Fazė","","","1~","1~","1~","1~","1~","1~","1~"]
["","Dažnis","","Hz","50","50","50","50","50","50","50"]
["","Įtampa","","V","220-240","220-240","220-240","220-240","220-240","220-240","220-240"]