{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":44,"n_cols":5,"rows_kept":44,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FLXS-B9"]
[]
[]
[]
[]
["","","","","FLXS35BAVMB9"]
["Garso slėgio lygis","Šildymas","Aukštas","dBA","46"]
["","","Tylus veikimas","dBA","30"]
["","","Žemas","dBA","33"]
["","Aušinimas","Tylus veikimas","dBA","29"]
["","","Žemas","dBA","32"]
["","","Aukštas","dBA","38"]
["","","Nom.","dBA","36"]
["","Aušinimas","Nom.","dBA","35"]
["Standartiniai priedai","Įrengimo vadovas","","","1"]
["","Eksploatavimo vadovas","","","1"]
["","Infraraudonųjų spindulių nuotolinio valdymo pultelis","","","1"]
["","AAA sausosios baterijos","","","2"]
["","Nuotolinio valdymo pulto laikiklis","","","1"]
["","Pritvirtinimo plokštė","","","1"]
["","Šilumos izoliacinis vamzdis (aušinimo medžiagos vamzdis)","","","8"]
["","Oro gryninimo filtras","","","1"]
["","Fotokatalizatoriaus kvapus šalinantis filtras","","","1"]
["","Šoninis dangtis","","","2"]
["","Rišamoji juosta","","","4"]
["Valdymo sistemos","Infrared remote control","","","ARC433B67"]
["Vamzdžių jungtys","Skysčių vamzdis","OD","mm","6.35"]
["","Dujos","Iš. diam.","mm","9.5"]
["","Drenažo vamzdis","","","18"]
["Garso galingumo lygis","Vėsinimas","","dBA","53"]
["","Šildymas","","dBA","59"]
["Matmenys","Vienetas","Plotis","mm","1,050"]
["","","Gylis","mm","200"]
["","","Aukštis","mm","490"]
["Korpusas","Colour","","","Migdolo balta spalva"]
["Svoris","Įrenginys","","kg","16"]
["Power supply","Phase","","","1~"]
["","Dažnis","","Hz","50"]
["","Pavadinimas","","","VM"]
["","Įtampa","","V","220-240"]
["Pastabos","","","","(1) - 220 V"]
["","","","","(2) - 230 V"]
["","","","","(3) - 240 V"]
["","","","","(4) - Kai sujungtas su sudėtinės sistemos išoriniu įrenginiu, žr. sudėtinio išorinio įrenginio specifikacijas prie kurios jungsite."]