{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":34,"n_cols":8,"rows_kept":34,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FNQ-A"]
[]
[]
[]
[]
["","","","","FNQ25A2VEB","FNQ35A2VEB","FNQ50A2VEB","FNQ60A2VEB"]
["Garso slėgio lygis","Šildymas","Aukštas","dBA","33","33","36","36"]
["","","Nom.","dBA","31","31","33","33"]
["","","Žemas","dBA","28","28","30","30"]
["","Aušinimas","Žemas","dBA","28","28","30","30"]
["","","Aukštas","dBA","33","33","36","36"]
["","","Nom.","dBA","31","31","33","33"]
["Šaltnešis","GWP","","","2,087.5","2,087.5","2,087.5","2,087.5"]
["Kontrolės sistemos","Wired remote control","","","BRC1D52, BRC1E52A/B","BRC1D52, BRC1E52A/B","BRC1D52, BRC1E52A/B","BRC1D52, BRC1E52A/B"]
["","Infrared remote control","","","BRC4C65","BRC4C65","BRC4C65","BRC4C65"]
["Aušinimo galingumas","Bendras pajėgumas","Nom.","kW","2.6","3.4","5.0","6.0"]
["Vamzdžių jungtys","Skystis","OD","mm","6.35","6.35","6.35","6.35"]
["","Dujos","Iš. diam.","mm","9.52","9.52","12.7","12.7"]
["","Drenažo vamzdis","","","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)"]
["Sound power level","Vėsinimas","","dBA","53","53","56","56"]
["Matmenys","Įrenginys","Plotis","mm","790","790","1,190","1,190"]
["","","Gylis","mm","200","200","200","200"]
["","","Aukštis","mm","620, 720 (2)","620, 720 (2)","620, 720 (2)","620, 720 (2)"]
["Korpusas","Medžiaga","","","Galvanizuoto plieno plokštė","Galvanizuoto plieno plokštė","Galvanizuoto plieno plokštė","Galvanizuoto plieno plokštė"]
["","Spalva","","","Nedažytas","Nedažytas","Nedažytas","Nedažytas"]
["Svoris","Įrenginys","","kg","23","23","30","30"]
["Ventiliatorius","Išorinis statinis slėgis","Aukštas","Pa","48","48","49","49"]
["","","Nom.","Pa","30","30","40","40"]
["Šildymo galingumas","Bendras pajėgumas","Nom.","kW","3.2","4.0","5.8","7.0"]
["Power supply","Fazė","","","1~","1~","1~","1~"]
["","Dažnis","","Hz","50/60","50/60","50/60","50/60"]
["","Įtampa","","V","220-240/220","220-240/220","220-240/220","220-240/220"]
["Pastabos","","","","(1) - Garso galios lygis yra absoliuti reikšmė nurodanti galią, kurią sukuria garso šaltinis.","(1) - Garso galios lygis yra absoliuti reikšmė nurodanti galią, kurią sukuria garso šaltinis.","(1) - Garso galios lygis yra absoliuti reikšmė nurodanti galią, kurią sukuria garso šaltinis.","(1) - Garso galios lygis yra absoliuti reikšmė nurodanti galią, kurią sukuria garso šaltinis."]
["","","","","(2) - Įskaitant montavimo kojas","(2) - Įskaitant montavimo kojas","(2) - Įskaitant montavimo kojas","(2) - Įskaitant montavimo kojas"]