{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":45,"n_cols":10,"rows_kept":45,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTX-GV"]
[]
[]
[]
[]
["","","","","FTX50GV1B","FTX60GV1B","FTX71GV1B","FTX20GV1B (Archived)","FTX25GV1B (Archived)","FTX35GV1B (Archived)"]
["Garso slėgio lygis","Šildymas","Aukštas","dBA","42","44","46","39","40","41"]
["","","Tylus veikimas","dBA","30","32","34","25","25","26"]
["","","Žemas","dBA","33","35","37","28","28","29"]
["","Aušinimas","Tylus veikimas","dBA","31","33","34","22","22","23"]
["","","Žemas","dBA","34","36","37","25","26","27"]
["","","Aukštas","dBA","43","45","46","39","40","41"]
["","","Nom.","dBA","38","40","42","34","34","35"]
["","Aušinimas","Nom.","dBA","39","41","42","33","33","34"]
["Standartiniai priedai","Įrengimo vadovas","","","1","1","1","1","1","1"]
["","Eksploatavimo vadovas","","","1","1","1","1","1","1"]
["","Belaidis nuotolinis valdymas","","","1","1","1","1","1","1"]
["","Elementai","","","2","2","2","2","2","2"]
["","Nuotolinio valdymo pulto laikiklis","","","1","1","1","1","1","1"]
["","Pritvirtinimo plokštė","","","1","1","1","1","1","1"]
["","Vidiniam įrenginiu skirtas tvirtinimo varžtas","","","","","","2","2","2"]
["","Titano apatito fotokatalizatoriaus oro gryninimo filtras","","","2","2","2","2","2","2"]
["Control systems","Infrared remote control","","","ARC433B70","ARC433B70","ARC433B70"]
["Vamzdžių jungtys","Skystis","OD","mm","6.35","6.35","6.35","6.35","6.35","6.35"]
["","Dujos","Iš. diam.","mm","12.7","12.7","15.9","9.52","9.52","9.52"]
["","Drenažo vamzdis","","","18","18","18","18","18","18"]
["Tiekiamas galingumas","Vėsinimas","Nom.","kW","0.034","0.040 (2), 0.040 (3), 0.040 (4)","0.045 (2), 0.045 (3), 0.045 (4)"]
["","Šildymas","Nom.","kW","0.036","0.045 (2), 0.045 (3), 0.045 (4)","0.060 (2), 0.060 (3), 0.06 (4)"]
["Sound power level","Vėsinimas","","dBA","59","60","63","55","56","57"]
["","Šildymas","","dBA","58","59","62","55","56","57"]
["Matmenys","Įrenginys","Plotis","mm","1,050","1,050","1,050","770","770","770"]
["","","Gylis","mm","238","238","238","198","198","198"]
["","","Aukštis","mm","290","290","290","283","283","283"]
["Casing","Spalva","","","Balta spalva","Balta spalva","Balta spalva","Balta spalva","Balta spalva","Balta spalva"]
["Weight","Įrenginys","","kg","12","12","12","7","7","7"]
["Power supply","Phase","","","1~","1~","1~","1~","1~","1~"]
["","Dažnis","","Hz","50","50","50","50","50","50"]
["","Pavadinimas","","","V1","V1","V1","V1","V1","V1"]
["","Įtampa","","V","220-240","220-240","220-240","220-240","220-240","220-240"]
["Standartiniai priedai","Vidinės įrangos pritvirtinimo varžtai","","","2","2"]
["Pastabos","","","","(1) - SL: tyli ventiliatoriaus oro srauto dažnio nustatymuose","(1) - SL: tyli ventiliatoriaus oro srauto dažnio nustatymuose","(1) - SL: tyli ventiliatoriaus oro srauto dažnio nustatymuose"]
["","","","","(2) - 220 V","(2) - 220 V","(2) - 220 V"]
["","","","","(3) - 230 V","(3) - 230 V","(3) - 230 V"]
["","","","","(4) - 240 V","(4) - 240 V","(4) - 240 V"]
["Standartiniai priedai","Vidaus įrenginių tvirtinimo varžtai (M4 x 12L)","","","","","2"]