{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":92,"n_cols":10,"rows_kept":92,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXA-AW"]
[]
[]
[]
[]
["","","","","","FTXA20A2V1BW","FTXA25A2V1BW","FTXA35A2V1BW","FTXA42A2V1BW","FTXA50A2V1BW"]
["Garso slėgio lygis","Šildymas","","Aukštas","dBA","39","40","41","","46"]
["","","","Vidutinis","dBA","32","33","33","","42"]
["","","","Tylus veikimas","dBA","19","19","19","","24"]
["","","","Žemas","dBA","25","25","25","","33"]
["","Aušinimas","","Vidutinis","dBA","32","33","33","","39"]
["","","","Tylus veikimas","dBA","19","19","19","","24"]
["","","","Žemas","dBA","25","25","25","","31"]
["","","","Aukštas","dBA","39","40","41","","46"]
["Standartiniai priedai","Įrengimo vadovas","","","","1","1","1","","1"]
["","Eksploatavimo vadovas","","","","1","1","1","","1"]
["","Oro filtras","","","","2","2","2","","2"]
["","Infraraudonųjų spindulių nuotolinio valdymo pultelis","","","","1","1","1","","1"]
["","Nuotolinio valdymo valdiklio montavimo plokštė","","","","1","1","1","","1"]
["","Sraigto maišas","","","","1","1","1","","1"]
["","Sraigto apdangalas","","","","1","1","1","","1"]
["","AAA sausosios baterijos","","","","2","2","2","","2"]
["","Bendrosios saugos priemonės","","","","1","1","1","","1"]
["Aušinimo medžiaga","GWP","","","","675.0","675.0","675.0","","675.0"]
["Valdymo sistemos","Wired remote control","","","","BRC073","BRC073","BRC073","","BRC073"]
["","Infrared remote control","","","","ARC466A58","ARC466A58","ARC466A58","","ARC466A58"]
["Piping connections","Skysčių vamzdis","","OD","mm","6.35","6.35","6.35","","6.35"]
["","Dujos","","Iš. diam.","mm","9.50","9.50","9.50","","12.70"]
["","Drenažo vamzdis","","","","18","18","18","","18"]
["Galios įvestis","Aušinimas","","Nom.","kW","0.020","0.022","0.023","","0.030"]
["","Šildymas","","Nom.","kW","0.020","0.020","0.022","","0.039"]
["Garso galingumo lygis","Vėsinimas","","","dBA","57","57","60","","60"]
["Matmenys","Vienetas","","Plotis","mm","798","798","798","","798"]
["","","","Gylis","mm","189","189","189","","189"]
["","","","Aukštis","mm","295","295","295","","295"]
["Korpusas","Spalva","","","","Balta spalva","Balta spalva","Balta spalva","","Balta spalva"]
["Weight","Įrenginys","","","kg","11.50","11.50","11.50","","11.50"]
["Ventiliatorius","Oro debitas","Šildymas","Didelis","m³/min.","10.9","11.1","11.5","","15.1"]
["","","","Vidutinis","m³/min.","8.7","9.0","9.0","","11.1"]
["","","","Mažas","m³/min.","6.4","6.4","6.4","","8.2"]
["","","","Tylus veikimas","m³/min.","4.5","4.5","4.5","","5.7"]
["","","Vėsinimas","Mažas","m³/min.","6.1","6.1","6.1","","7.6"]
["","","","Vidutinis","m³/min.","8.2","8.6","8.6","","10.4"]
["","","","Didelis","m³/min.","11.0","11.5","11.9","","13.5"]
["","","","Tylus veikimas","m³/min.","4.6","4.6","4.6","","5.2"]
["Power supply","Fazė","","","","1~","1~","1~","","1~"]
["","Pavadinimas","","","","V1","V1","V1","","V1"]
["","Dažnis","","","Hz","50","50","50","","50"]
["","Įtampa","","","V","220-240","220-240","220-240","","220-240"]
["Tiekiama galia","Aušinimas","","Nom.","kW","","","","0.028"]
["","Šildymas","","Nom.","kW","","","","0.036"]
["Korpusas","Spalva","","","","","","","Balta"]
["Matmenys","Įrenginys","","Aukštis","mm","","","","295"]
["","","","Plotis","mm","","","","798"]
["","","","Gylis","mm","","","","189"]
["Svoris","Įrenginys","","","kg","","","","11.50"]
["Ventiliatorius","Oro debitas","Aušinimas","Didelis","m³/min.","","","","13.1"]
["","Oro srauto greitis","Vėsinimas","Vidutinis","m³/min.","","","","9.8"]
["","","","Mažas","m³/min.","","","","7.2"]
["","","","Tylus veikimas","m³/min.","","","","4.6"]
["","","Šildymas","Didelis","m³/min.","","","","14.6"]
["","Oro srauto greitis","Šildymas","Vidutinis","m³/min.","","","","10.5"]
["","","Šildymas","Mažas","m³/min.","","","","7.7"]
["","","","Tylus veikimas","m³/min.","","","","5.2"]
["Garso galingumo lygis","Vėsinimas","","","dBA","","","","60"]
["Garso slėgio lygis","Aušinimas","","Aukštas","dBA","","","","45"]
["","Vėsinimas","","Vidutinis","dBA","","","","37"]
["","","","Žemas","dBA","","","","29"]
["","","","Tylus veikimas","dBA","","","","21"]
["","Šildymas","","Aukštas","dBA","","","","45"]
["","","","Vidutinis","dBA","","","","37"]
["","","","Žemas","dBA","","","","29"]
["","","","Tylus veikimas","dBA","","","","21"]
["Aušinimo medžiaga","GWP","","","","","","","675.0"]
["Vamzdžių jungtys","Skystis","","OD","mm","","","","6.35"]
["","Dujos","","Iš. diam.","mm","","","","12.70"]
["","Drenažas","","","","","","","18"]
["Valdymo sistemos","Nuotolinis infraraudonųjų spindulių pultelis","","","","","","","ARC466A58"]
["","Laidinis nuotolinio valdymo pultelis","","","","","","","BRC073"]
["Standartiniai priedai","Installation manual","","","","","","","1"]
["","Screw cover","","","","","","","1"]
["","AAA dry-cell batteries","","","","","","","2"]
["","General safety precautions","","","","","","","1"]
["","Operation manual","","","","","","","1"]
["","Air filter","","","","","","","2"]
["","Infrared remote control","","","","","","","1"]
["","Remote controller mounting plate","","","","","","","1"]
["","Screw bag","","","","","","","1"]
["El. tiekimas","Pavadinimas","","","","","","","V1"]
["","Fazė","","","","","","","1~"]
["Maitinimas","Dažnis","","","Hz","","","","50"]
["","Įtampa","","","V","","","","220-240"]