{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":38,"n_cols":6,"rows_kept":38,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXF-B"]
[]
[]
[]
[]
["","","","","FTXF20B5V1B","FTXF25B5V1B"]
["Garso slėgio lygis","Šildymas","Aukštas","dBA","39","40"]
["","","Vidutinis","dBA","34","34"]
["","","Tylus veikimas","dBA","21","21"]
["","","Žemas","dBA","28","28"]
["","Aušinimas","Vidutinis","dBA","33","33"]
["","","Tylus veikimas","dBA","20","20"]
["","","Žemas","dBA","25","26"]
["","","Aukštas","dBA","39","40"]
["Standartiniai priedai","Įrengimo vadovas","","","1","1"]
["","Eksploatavimo vadovas","","","1","1"]
["","Infraraudonųjų spindulių nuotolinio valdymo pultelis","","","1","1"]
["","AAA sausosios baterijos","","","2","2"]
["","Nuotolinio valdymo pulto laikiklis","","","1","1"]
["","Pritvirtinimo plokštė","","","1","1"]
["","Vidinės įrangos pritvirtinimo varžtai","","","2","2"]
["Valdymo sistemos","Wired remote control","","","BRC944B2, BRC073A1","BRC944B2, BRC073A1"]
["","Nuotolinis valdymas infraraudonaisiais spinduliais","","","ARC470A1","ARC470A1"]
["Vamzdžių jungtys","Skystis","OD","mm","6.35","6.35"]
["","Dujų vamzdis","Iš. diam.","mm","9.50","9.50"]
["","Drenažo vamzdis","","","18","18"]
["Tiekiamas galingumas","Aušinimas","Nom.","kW","0.017","0.019"]
["","Šildymas","Nom.","kW","0.020","0.020"]
["Garso galingumo lygis","Vėsinimas","","dBA","55","55"]
["","Šildymas","","dBA","55","55"]
["Matmenys","Vienetas","Plotis","mm","770","770"]
["","","Gylis","mm","225","225"]
["","","Aukštis","mm","286","286"]
["Korpusas","Spalva","","","Balta spalva","Balta spalva"]
["Svoris","Įrenginys","","kg","8.50","8.50"]
["Power supply","Fazė","","","1~","1~"]
["","Dažnis","","Hz","50","50"]
["","Įtampa","","V","220-240","220-240"]