{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":51,"n_cols":9,"rows_kept":51,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXG-LW"]
[]
[]
[]
[]
["","","","","","FTXG20LV1BW","FTXG25LV1BW","FTXG35LV1BW","FTXG50LV1BW"]
["Tiekiama galia","Aušinimas","","Nom.","kW","0.023, 0.023, 0.023","0.023, 0.023, 0.023","0.033, 0.033, 0.033","0.033, 0.033, 0.033"]
["","Šildymas","","Nom.","kW","0.031, 0.031, 0.031","0.033, 0.033, 0.033","0.042, 0.042, 0.042","0.043, 0.043, 0.043"]
["Korpusas","Spalva","","","","Balta","Balta","Balta","Balta"]
["Matmenys","Įrenginys","","Aukštis","mm","303","303","303","303"]
["","","","Plotis","mm","998","998","998","998"]
["","","","Gylis","mm","212","212","212","212"]
["Svoris","Įrenginys","","","kg","12.0","12.0","12.0","12.0"]
["Ventiliatorius","Oro debitas","Aušinimas","Didelis","m³/min.","8.9","8.9","10.9","10.9"]
["","Oro srauto greitis","Vėsinimas","Vidutinis","m³/min.","6.6","6.6","7.8","8.9"]
["","","","Mažas","m³/min.","4.4","4.4","4.8","6.8"]
["","","","Tylus veikimas","m³/min.","2.6","2.6","2.9","3.6"]
["","","Šildymas","Didelis","m³/min.","10.2","11.0","12.4","12.6"]
["","Oro srauto greitis","Šildymas","Vidutinis","m³/min.","8.4","8.6","9.6","10.5"]
["","","Šildymas","Mažas","m³/min.","6.3","6.3","6.9","8.1"]
["","","","Tylus veikimas","m³/min.","3.8","3.8","4.1","5.0"]
["Garso galingumo lygis","Vėsinimas","","","dBA","54","54","59","60"]
["","Šildymas","","","dBA","56","56","59","60"]
["Garso slėgio lygis","Aušinimas","","Aukštas","dBA","38","38","45","46"]
["","Vėsinimas","","Vidutinis","dBA","32","32","34","40"]
["","","","Žemas","dBA","25","25","26","35"]
["","","","Tylus veikimas","dBA","19","19","20","25"]
["","Šildymas","","Aukštas","dBA","40","41","45","47"]
["","","","Vidutinis","dBA","34","34","37","41"]
["","","","Žemas","dBA","28","28","29","35"]
["","","","Tylus veikimas","dBA","19","19","20","25"]
["Vamzdžių jungtys","Skystis","","OD","mm","6.35","6.35","6.35","6.35"]
["","Dujos","","Iš. diam.","mm","9.50","9.50","9.50","12.7"]
["","Drenažas","","","","18","18","18","18"]
["Control systems","Infrared remote control","","","","ARC466A9","ARC466A9","ARC466A9","ARC466A9"]
["Standartiniai priedai","Installation manual","","","","1","1","1","1"]
["","Wireless remote control","","","","1","1","1","1"]
["","Screw cover","","","","2","2","2","2"]
["","Operation manual","","","","1","1","1","1"]
["","Titanium apatite deodorizing filter","","","","2","2","2","2"]
["","Batteries","","","","2","2","2","2"]
["","Indoor unit fixing screws","","","","2","2","2","2"]
["","Mounting plate","","","","1","1","1","1"]
["","Remote control holder","","","","1","1","1","1"]
["El. tiekimas","Pavadinimas","","","","V1","V1","V1","V1"]
["","Fazė","","","","1~","1~","1~","1~"]
["Maitinimas","Dažnis","","","Hz","50","50","50","50"]
["","Įtampa","","","V","220-240","220-240","220-240","220-240"]
["Pastabos","","","","","(1) - 220 V","(1) - 220 V","(1) - 220 V","(1) - 220 V"]
["","","","","","(2) - 230 V","(2) - 230 V","(2) - 230 V","(2) - 230 V"]
["","","","","","(3) - 240 V","(3) - 240 V","(3) - 240 V","(3) - 240 V"]