{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":52,"n_cols":10,"rows_kept":52,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXJ-AW9"]
[]
[]
[]
[]
["","","","","","FTXJ20A2V1BW9","FTXJ25A2V1BW9","FTXJ35A2V1BW9","FTXJ42A2V1BW9","FTXJ50A2V1BW9"]
["Tiekiama galia","Aušinimas","","Nom.","kW","0.02","0.022","0.024","0.028","0.031"]
["","Šildymas","","Nom.","kW","0.021","0.022","0.024","0.036","0.039"]
["Korpusas","Spalva","","","","Balta","Balta","Balta","Balta","Balta"]
["Matmenys","Įrenginys","","Aukštis","mm","305","305","305","305","305"]
["","","","Plotis","mm","900","900","900","900","900"]
["","","","Gylis","mm","212","212","212","212","212"]
["Svoris","Įrenginys","","","kg","12","12","12","12","12"]
["Ventiliatorius","Oro debitas","Aušinimas","Didelis","m³/min.","11","11.4","11.8","13","13.5"]
["","Oro srauto greitis","Vėsinimas","Vidutinis","m³/min.","8.4","8.6","8.6","9.5","10.4"]
["","","","Mažas","m³/min.","6","6","6","7.2","7.6"]
["","","","Tylus veikimas","m³/min.","4.6","4.6","4.6","4.6","5.2"]
["","","Šildymas","Didelis","m³/min.","11.1","11.3","11.7","14.4","15"]
["","Oro srauto greitis","Šildymas","Vidutinis","m³/min.","8.7","9","9","10.5","11.1"]
["","","Šildymas","Mažas","m³/min.","6.4","6.4","6.4","7.7","8.2"]
["","","","Tylus veikimas","m³/min.","4.6","4.6","4.6","5.2","5.7"]
["Garso galingumo lygis","Vėsinimas","","","dBA","57","57","60","60","60"]
["Garso slėgio lygis","Aušinimas","","Aukštas","dBA","39","40","41","45","46"]
["","Vėsinimas","","Vidutinis","dBA","32","33","33","37","39"]
["","","","Žemas","dBA","25","25","25","29","31"]
["","","","Tylus veikimas","dBA","19","19","19","21","24"]
["","Šildymas","","Aukštas","dBA","39","40","41","45","46"]
["","","","Vidutinis","dBA","32","33","33","37","42"]
["","","","Žemas","dBA","25","25","25","29","33"]
["","","","Tylus veikimas","dBA","19","19","19","21","24"]
["Aušinimo medžiaga","GWP","","","","675","675","675","675","675"]
["Vamzdžių jungtys","Skystis","","OD","mm","6.35","6.35","6.35","6.35","6.35"]
["","Dujos","","Iš. diam.","mm","9.5","9.5","9.5","12.7","12.7"]
["","Drenažas","","","","18","18","18","18","18"]
["Valdymo sistemos","Nuotolinis infraraudonųjų spindulių pultelis","","","","ARC488A1W","ARC488A1W","ARC488A1W","ARC488A1W","ARC488A1W"]
["","Laidinis nuotolinio valdymo pultelis","","","","BRC073A1","BRC073A1","BRC073A1","BRC073A1","BRC073A1"]
["Standartiniai priedai","Installation manual","","","","1","1","1","1","1"]
["","Wireless remote control","","","","1","1","1","1","1"]
["","Screw cover","","","","2","2","2","2","2"]
["","AAA dry-cell batteries","","","","2","2","2","2","2"]
["","General safety precautions","","","","1","1","1","1","1"]
["","Operation manual","","","","1","1","1","1","1"]
["","Titanium apatite deodorizing filter","","","","1","1","1","1","1"]
["","Silver particle filter","","","","1","1","1","1","1"]
["","Remote control holder","","","","1","1","1","1","1"]
["","Screw bag","","","","1","1","1","1","1"]
["El. tiekimas","Pavadinimas","","","","V1","V1","V1","V1","V1"]
["","Fazė","","","","1~","1~","1~","1~","1~"]
["Maitinimas","Dažnis","","","Hz","50","50","50","50","50"]
["","Įtampa","","","V","220-240","220-240","220-240","220-240","220-240"]
["Pastabos","","","","","(1) - Aušinimas: vidaus temp. 27 °CDB, 19,0 °CWB; lauko temp. 35 °CDB, 24 °CWB; ekvivalentinis vamzdyno ilgis: 5 m","(1) - Aušinimas: vidaus temp. 27 °CDB, 19,0 °CWB; lauko temp. 35 °CDB, 24 °CWB; ekvivalentinis vamzdyno ilgis: 5 m","(1) - Aušinimas: vidaus temp. 27 °CDB, 19,0 °CWB; lauko temp. 35 °CDB, 24 °CWB; ekvivalentinis vamzdyno ilgis: 5 m","(1) - Aušinimas: vidaus temp. 27 °CDB, 19,0 °CWB; lauko temp. 35 °CDB, 24 °CWB; ekvivalentinis vamzdyno ilgis: 5 m","(1) - Aušinimas: vidaus temp. 27 °CDB, 19,0 °CWB; lauko temp. 35 °CDB, 24 °CWB; ekvivalentinis vamzdyno ilgis: 5 m"]
["","","","","","(2) - Šildymas: vidaus temp. 20 °CDB; lauko temp. 7 °CDB, 6 °CWB; ekvivalentinis aušinimo medžiagos vamzdyno ilgis: 5 m","(2) - Šildymas: vidaus temp. 20 °CDB; lauko temp. 7 °CDB, 6 °CWB; ekvivalentinis aušinimo medžiagos vamzdyno ilgis: 5 m","(2) - Šildymas: vidaus temp. 20 °CDB; lauko temp. 7 °CDB, 6 °CWB; ekvivalentinis aušinimo medžiagos vamzdyno ilgis: 5 m","(2) - Šildymas: vidaus temp. 20 °CDB; lauko temp. 7 °CDB, 6 °CWB; ekvivalentinis aušinimo medžiagos vamzdyno ilgis: 5 m","(2) - Šildymas: vidaus temp. 20 °CDB; lauko temp. 7 °CDB, 6 °CWB; ekvivalentinis aušinimo medžiagos vamzdyno ilgis: 5 m"]