{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":26,"n_cols":5,"rows_kept":26,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXJ-MS / 4MXM-A8"]
[]
[]
[]
[]
["","","","","FTXJ20MV1BS / FTXJ20MV1BS / FTXJ20MV1BS / FTXJ20MV1BS / 4MXM80A2V1B8"]
["Aušinimo galingumas","Nom.","","kW","7.50"]
["Šildymo galingumas","Nom.","","kW","10.00"]
["Nominalus efektyvumas","EER","","","4.13"]
["","COP","","","3.32"]
["","Metinis energijos sunaudojimas","","kWh","908"]
["Vardinis našumas","Energijos suvartojimo ženklinimo direktyva","Vėsinimas","","A"]
["","","Šildymas","","C"]
["Patalpos vėsinimas","Energijos efektyvumo klasė","","","A++"]
["","Vėsinimas","Pdesign","kW","7.50"]
["","SEER","","","6.92"]
["","Metinės energijos sąnaudos","","kWh/m.","380"]
["Patalpos šildymas (vidutinis klimatas)","Energijos efektyvumo klasė","","","A+"]
["","Pajėgumas","Pdesign","kW","6.46"]
["","SCOP/A","","","4.02"]
["","Pdh Šildymo pajėgumas esant –10°","","kW","5.28"]
["","Metinės energijos sąnaudos","","kWh/m.","2,245"]
["Pastabos","","","","(1) - Nominalus aušinimo galingumas yra pagrįstas: patalpų temp.: 27°CDB/19°CWB, išorinė temperatūra: 35 °CDB, ekvivalentinis šaltnešio vamzdynas: 5 m, aukščio skirtumas: 0 m."]
["","","","","(2) - Nominali šildymo galia nustatyta remiantis: vidaus temperatūra: 20 °CDB, lauko temperatūra: 7 °CDB, 6 °CWB, ekvivalentinis aušinimo medžiagos vamzdyno ilgis: 5 m, aukščių skirtumas: 0 m."]
["","","","","(3) - Žr. specialų darbinio diapazono brėžinį"]
["","","","","(4) - Žr. atskirą elektros duomenų brėžinį"]