{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":17,"n_cols":5,"rows_kept":17,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXJ-MW / 3MXM-N7"]
[]
[]
[]
[]
["","","","","FTXJ20MV1BW / FTXJ20MV1BW / 3MXM40N2V1B7"]
["Aušinimo galingumas","Nom.","","kW","4.00"]
["Vardinis našumas","Metinis energijos sunaudojimas","","kWh","482"]
["","EER","","","4.15"]
["","COP","","","3.95"]
["","Energijos suvartojimo ženklinimo direktyva","Vėsinimas","","A"]
["","","Šildymas","","A"]
["Šildymo galingumas","Nom.","","kW","4.60"]
["Pastabos","","","","(1) - Nominalus aušinimo galingumas yra pagrįstas: patalpų temperatūra: 27°CDB/19°CWB, išorinė temperatūra: 35 °CDB, ekvivalentinis šaltnešio vamzdynas: 5 m, aukščio skirtumas: 0 m."]
["","","","","(2) - Nominali šildymo galia nustatyta remiantis: vidaus temperatūra: 20 °CDB, lauko temperatūra: 7 °CDB, 6 °CWB, ekvivalentinis aušinimo medžiagos vamzdyno ilgis: 5 m, aukščių skirtumas: 0 m."]
["","","","","(3) - Žr. specialų darbinio diapazono brėžinį"]
["","","","","(4) - Žr. atskirą elektros duomenų brėžinį"]