{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":50,"n_cols":7,"rows_kept":50,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXL-JV"]
[]
[]
[]
[]
["","","","","","FTXL25J2V1B","FTXL35J2V1B"]
["Tiekiama galia","Aušinimas","","Nom.","kW","0.040, 0.040, 0.040","0.040, 0.040, 0.040"]
["","Šildymas","","Nom.","kW","0.040, 0.040, 0.040","0.040, 0.040, 0.040"]
["Korpusas","Spalva","","","","Balta","Balta"]
["Matmenys","Įrenginys","","Aukštis","mm","283","283"]
["","","","Plotis","mm","770","770"]
["","","","Gylis","mm","198","198"]
["Svoris","Įrenginys","","","kg","8.00","8.00"]
["Ventiliatorius","Oro debitas","Aušinimas","Didelis","m³/min.","9.3","9.3"]
["","Oro srauto greitis","Vėsinimas","Vidutinis","m³/min.","7.7","7.7"]
["","","","Mažas","m³/min.","6.1","6.1"]
["","","","Tylus veikimas","m³/min.","4.9","4.9"]
["","","Šildymas","Didelis","m³/min.","10.1","10.1"]
["","Oro srauto greitis","Šildymas","Vidutinis","m³/min.","8.4","8.4"]
["","","Šildymas","Mažas","m³/min.","6.7","6.7"]
["","","","Tylus veikimas","m³/min.","5.7","5.7"]
["Garso galingumo lygis","Vėsinimas","","","dBA","57","57"]
["","Šildymas","","","dBA","57","57"]
["Garso slėgio lygis","Aušinimas","","Aukštas","dBA","41","41"]
["","Vėsinimas","","Vidutinis","dBA","34","34"]
["","","","Žemas","dBA","27","27"]
["","","","Tylus veikimas","dBA","23","23"]
["","Šildymas","","Aukštas","dBA","41","41"]
["","","","Vidutinis","dBA","35","35"]
["","","","Žemas","dBA","29","29"]
["","","","Tylus veikimas","dBA","26","26"]
["Vamzdžių jungtys","Skystis","","OD","mm","6.35","6.35"]
["","Dujos","","Iš. diam.","mm","9.50","9.50"]
["","Drenažas","","","","18","18"]
["Valdymo sistemos","Infrared remote control","","","","ARC433A87, ARC466A9","ARC433A87, ARC466A9"]
["Standartiniai priedai","Installation manual","","","","1","1"]
["","Wireless remote control","","","","1","1"]
["","Operation manual","","","","1","1"]
["","Titanium apatite deodorizing filter","","","","2","2"]
["","Batteries","","","","2","2"]
["","Indoor unit fixing screws","","","","2","2"]
["","Mounting plate","","","","1","1"]
["","Remote control holder","","","","1","1"]
["El. tiekimas","Pavadinimas","","","","V1","V1"]
["","Fazė","","","","1~","1~"]
["Maitinimas","Dažnis","","","Hz","50","50"]
["","Įtampa","","","V","220-240","220-240"]
["Pastabos","","","","","(1) - 220 V","(1) - 220 V"]
["","","","","","(2) - 230 V","(2) - 230 V"]
["","","","","","(3) - 240 V","(3) - 240 V"]