{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":42,"n_cols":7,"rows_kept":42,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXP-M9 / RXP-M"]
[]
[]
[]
[]
["","","","","FTXP20M5V1B9 / RXP20M5V1B","FTXP25M5V1B9 / RXP25M5V1B","FTXP35M5V1B9 / RXP35M5V1B"]
["Outdoor unit","","","","RXP20M5V1B","RXP25M5V1B","RXP35M5V1B"]
["Aušinimo galingumas","Min.","","kW","","1.3"]
["","Nom.","","kW","","2.50"]
["","Maks.","","kW","","3.0"]
["Šildymo galingumas","Min.","","kW","","1.30"]
["","Nom.","","kW","","3.00"]
["","Maks.","","kW","","4.00"]
["Vardinis našumas","Annual energy consumption","","kWh","","326"]
["","COP","","","","4.36"]
["","EER","","","","3.83"]
["","Energijos suvartojimo ženklinimo direktyva","Vėsinimas","","","A"]
["","","Šildymas","","","A"]
["Pastabos","","","","","(1) - Nominalus aušinimo galingumas yra pagrįstas: patalpų temperatūra: 27°CDB/19°CWB, išorinė temperatūra: 35 °CDB, ekvivalentinis šaltnešio vamzdynas: 5 m, aukščio skirtumas: 0 m."]
["","","","","","(2) - Nominali šildymo galia nustatyta remiantis: vidaus temperatūra: 20 °CDB, lauko temperatūra: 7 °CDB, 6 °CWB, ekvivalentinis aušinimo medžiagos vamzdyno ilgis: 5 m, aukščių skirtumas: 0 m."]
["","","","","","(3) - Žr. atskirą elektros duomenų brėžinį"]
["Aušinimo galingumas","Min.","","kW","1.3","","1.3"]
["","Nom.","","kW","2.00","","3.50"]
["","Maks.","","kW","2.6","","4.0"]
["Šildymo galingumas","Min.","","kW","1.30","","1.30"]
["","Nom.","","kW","2.50","","4.00"]
["","Maks.","","kW","3.50","","4.80"]
["Nominalus efektyvumas","EER","","","4.02","","3.49"]
["","COP","","","4.77","","4.02"]
["","Metinis energijos sunaudojimas","","kWh","249"]
["Vardinis našumas","Energijos suvartojimo ženklinimo direktyva","Vėsinimas","","A","","A"]
["","","Šildymas","","A","","A"]
["Patalpos vėsinimas","Energijos efektyvumo klasė","","","A++","","A++"]
["","Vėsinimas","Pdesign","kW","2.00","","3.50"]
["","SEER","","","6.79","","6.62"]
["","Metinės energijos sąnaudos","","kWh/m.","103","","186"]
["Patalpos šildymas (vidutinis klimatas)","Energijos efektyvumo klasė","","","A++","","A++"]
["","Pajėgumas","Pdesign","kW","2.20","","2.80"]
["","SCOP/A","","","4.65","","4.64"]
["","Pdh Šildymo pajėgumas esant –10°","","kW","1.99","","2.33"]
["","Metinės energijos sąnaudos","","kWh/m.","662","","845"]
["Energijos naudojimo efektyvumo klasė","","","","A+++ ~ D","","A+++ ~ D"]