{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":48,"n_cols":8,"rows_kept":48,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXP-M9"]
[]
[]
[]
[]
["","","","","","FTXP20M5V1B9","FTXP25M5V1B9","FTXP35M5V1B9"]
["Tiekiama galia","Aušinimas","","Nom.","kW","0.019","0.02","0.032"]
["","Šildymas","","Nom.","kW","0.023","0.023","0.032"]
["Korpusas","Spalva","","","","Balta","Balta","Balta"]
["Matmenys","Įrenginys","","Aukštis","mm","286","286","286"]
["","","","Plotis","mm","770","770","770"]
["","","","Gylis","mm","225","225","225"]
["Svoris","Įrenginys","","","kg","8.5","8.5","9"]
["Ventiliatorius","Oro debitas","Aušinimas","Didelis","m³/min.","9.5","9.7","11.5"]
["","Oro srauto greitis","Vėsinimas","Vidutinis","m³/min.","7.4","7.7","8.3"]
["","","","Mažas","m³/min.","5.6","5.8","6.3"]
["","","","Tylus veikimas","m³/min.","4.2","4.2","4.5"]
["","","Šildymas","Didelis","m³/min.","10.4","10.4","11.5"]
["","Oro srauto greitis","Šildymas","Vidutinis","m³/min.","8.1","8.1","9"]
["","","Šildymas","Mažas","m³/min.","6.2","6.4","7"]
["","","","Tylus veikimas","m³/min.","5.2","5.2","5.3"]
["Garso galingumo lygis","Vėsinimas","","","dBA","55","55","58"]
["","Šildymas","","","dBA","55","55","58"]
["Garso slėgio lygis","Aušinimas","","Aukštas","dBA","39","40","43"]
["","Vėsinimas","","Vidutinis","dBA","33","33","34"]
["","","","Žemas","dBA","25","26","27"]
["","","","Tylus veikimas","dBA","19","19","20"]
["","Šildymas","","Aukštas","dBA","39","40","40"]
["","","","Vidutinis","dBA","34","34","35"]
["","","","Žemas","dBA","28","28","29"]
["","","","Tylus veikimas","dBA","21","21","21"]
["Vamzdžių jungtys","Skystis","","OD","mm","6.35","6.35","6.35"]
["","Dujos","","Iš. diam.","mm","9.5","9.5","9.5"]
["","Drenažas","","","","18","18","18"]
["Control systems","Infrared remote control","","","","ARC480A53","ARC480A53","ARC480A53"]
["Valdymo sistemos","Laidinis nuotolinio valdymo pultelis","","","","BRC944B2, BRC073A1","BRC944B2, BRC073A1","BRC944B2, BRC073A1"]
["Standartiniai priedai","Installation manual","","","","1","1","1"]
["","AAA dry-cell batteries","","","","2","2","2"]
["","Operation manual","","","","1","1","1"]
["","Titanium apatite deodorizing filter","","","","1","2","2"]
["","Silver particle filter","","","","1"]
["","Indoor unit fixing screws","","","","2","2","2"]
["","Infrared remote control","","","","1","1","1"]
["","Mounting plate","","","","1","1","1"]
["","Remote control holder","","","","1","1","1"]
["El. tiekimas","Fazė","","","","1~","1~","1~"]
["Maitinimas","Dažnis","","","Hz","50","50","50"]
["","Įtampa","","","V","220-240","220-240","220-240"]