{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":18,"n_cols":6,"rows_kept":18,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXS-G / RKS-F"]
[]
[]
[]
[]
["","","","","FTXS60GV1B / RKS60F3V1B","FTXS71GV1B / RKS71FAV1B"]
["Vėsinimo pajėgumas","Min.","","kW","1.7","2.3"]
["","Maks.","","kW","6.7","8.5"]
["","Nom.","","kW","6.0 (1)","7.1 (1)"]
["Vamzdžių jungtys","Skystis","OD","mm","6.35","6.35"]
["","Dujos","OD","mm","12.7","15.9"]
["","Drenažo vamzdis","OD","mm","18.0","18.0"]
["Vardinis našumas","Annual energy consumption","","kWh","995","1,175"]
["","EER","","","3.02","3.02"]
["","Energijos suvartojimo ženklinimo direktyva","Vėsinimas","","B","D"]
["Pastabos","","","","(1) - Aušinimas: vidaus temp. 27 °CDB, 19,0 °CWB; lauko temp. 35 °CDB, 24 °CWB; ekvivalentinis vamzdyno ilgis: 5 m","(1) - Aušinimas: vidaus temp. 27 °CDB, 19,0 °CWB; lauko temp. 35 °CDB, 24 °CWB; ekvivalentinis vamzdyno ilgis: 5 m"]
["","","","","(2) - Aušinimo pajėgumai yra bendri, įskaitant vidaus patalpų ventiliatoriaus kaitimo aušinimo mažinimą.","(2) - Nominalus efektyvumas: vėsinimas esant 35°/27° nominaliąja apkrova, šildymas esant 7°/20° nominaliąja apkrova"]
["","","","","(3) - Nominalus efektyvumas: vėsinimas esant 35°/27° nominaliąja apkrova, šildymas esant 7°/20° nominaliąja apkrova"]