{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":25,"n_cols":5,"rows_kept":25,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXS-G / RXS-L"]
[]
[]
[]
[]
["","","","","FTXS60GV1B / RXS60L2V1B"]
["Aušinimo galingumas","Min.","","kW","1.7"]
["","Maks.","","kW","6.7"]
["","Nom.","","kW","6.0"]
["Vamzdžių jungtys","Skystis","OD","mm","6.35"]
["","Dujos","Iš. diam.","mm","12.7"]
["","Drenažo vamzdis","OD","mm","18"]
["Vardinis našumas","Metinis energijos sunaudojimas","","kWh","995"]
["","EER","","","3.02"]
["","COP","","","3.43"]
["","Energijos suvartojimo ženklinimo direktyva","Vėsinimas","","B"]
["","","Šildymas","","B"]
["Šildymo galingumas","Nom.","","kW","7.0"]
["","Min.","","kW","1.7"]
["","Maks.","","kW","8.0"]
["Pastabos","","","","(1) - EER/COP pagal „Eurovent 2012“, skirta naudoti tik už ES ribų"]
["","","","","(2) - 220 V"]
["","","","","(3) - 230 V"]
["","","","","(4) - 240 V"]
["","","","","(5) - Nominalus efektyvumas: vėsinimas esant 35°/27° nominaliąja apkrova, šildymas esant 7°/20° nominaliąja apkrova"]