{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":85,"n_cols":12,"rows_kept":85,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXS-G"]
[]
[]
[]
[]
["","","","","","FTXS20G2V1B","FTXS25G2V1B","FTXS35G2V1B","FTXS42G2V1B","FTXS50G2V1B","FTXS60GV1B","FTXS71GV1B"]
["Garso slėgio lygis","Šildymas","","Aukštas","dBA","38","39","42","42","44","","46"]
["","","","Tylus veikimas","dBA","25","25","26","30","31","","34"]
["","","","Žemas","dBA","28","28","29","33","34","","37"]
["","Aušinimas","","Tylus veikimas","dBA","22","22","23","30","31","","34"]
["","","","Žemas","dBA","25","25","26","33","34","","37"]
["","","","Aukštas","dBA","38","38","42","42","43","","46"]
["","","","Nom.","dBA","33","34","36","38","39","","42"]
["","Aušinimas","","Nom.","dBA","32","32","34","38","39","","42"]
["Standartiniai priedai","Titano apatito fotokatalizatoriaus oro gryninimo filtras","","","","2","2","2","2","2"]
["","Eksploatavimo vadovas","","","","1","1","1","1","1","","1"]
["","Įrengimo vadovas","","","","1","1","1","1","1","","1"]
["","Belaidis nuotolinis valdymas","","","","1","1","1","1","1","","1"]
["","Elementai","","","","2","2","2","2","2","","2"]
["","Nuotolinio valdymo pulto laikiklis","","","","1","1","1","1","1","","1"]
["","Vidinės įrangos pritvirtinimo varžtai","","","","2","2","2","2","2","","2"]
["","Pritvirtinimo plokštė","","","","1","1","1","1","1","","1"]
["Kontrolės sistemos","Infrared remote control","","","","","","","","","","ARC452A3"]
["Piping connections","Liquid","","OD","mm","6.35","6.35","6.35","6.35","6.35","","6.35"]
["","Dujos","","Iš. diam.","mm","9.52","9.52","9.52","9.52","12.70","","15.9"]
["","Drain","","","","18","18","18","18","18","","18"]
["Tiekiamas galingumas","Aušinimas","","Nom.","kW","","","","","","","0.045 (2), 0.045 (3), 0.045 (4)"]
["","Šildymas","","Nom.","kW","","","","","","","0.060 (2), 0.060 (3), 0.060 (4)"]
["Garso galingumo lygis","Vėsinimas","","","dBA","54","54","58","58","59","","63"]
["","Šildymas","","","dBA","54","55","58","58","60","","62"]
["Matmenys","Vienetas","","Plotis","mm","800","800","800","800","800","","1,050"]
["","","","Depth","mm","215","215","215","215","215","","250"]
["","","","Aukštis","mm","295","295","295","295","295","","290"]
["Korpusas","Colour","","","","Balta spalva","Balta spalva","Balta spalva","Balta spalva","Balta spalva","","Balta spalva"]
["Svoris","Vienetas","","","kg","9","9","10","10","10","","12"]
["Power supply","Fazė","","","","1~","1~","1~","1~","1~","","1~"]
["","Dažnis","","","Hz","50","50","50","50","50","","50"]
["","Name","","","","V1","V1","V1","V1","V1","","V1"]
["","Įtampa","","","V","220-240","220-240","220-240","220-240","220-240","","220-240"]
["Pastabos","","","","","(1) - 220 V","(1) - 220 V","(1) - 220 V","(1) - 220 V","(1) - 220 V","(1) - 220 V","(1) - SL: tyli ventiliatoriaus oro srauto dažnio nustatymuose"]
["","","","","","(2) - 230 V","(2) - 230 V","(2) - 230 V","(2) - 230 V","(2) - 230 V","(2) - 230 V","(2) - 220 V"]
["","","","","","(3) - 240 V","(3) - 240 V","(3) - 240 V","(3) - 240 V","(3) - 240 V","(3) - 240 V","(3) - 230 V"]
["Ventiliatorius","Oro debitas","Aušinimas","Nom.","m³/min.","","","","","","16.0"]
["Garso slėgio lygis","Aušinimas","","Nom.","dBA","","","","","","41"]
["Ventiliatorius","Oro debitas","Šildymas","Nom.","m³/min.","","","","","","14.9"]
["Garso slėgio lygis","Šildymas","","Nom.","dBA","","","","","","40"]
["Tiekiama galia","Aušinimas","","Nom.","kW","","","","","","0.040 (4) (2) (3), 0.040 (4) (2) (3), 0.040 (4) (2) (3)"]
["","Šildymas","","Nom.","kW","","","","","","0.045 (4) (2) (3), 0.045 (4) (2) (3), 0.045 (4) (2) (3)"]
["Korpusas","Spalva","","","","","","","","","Balta"]
["Matmenys","Įrenginys","","Aukštis","mm","","","","","","290"]
["","","","Plotis","mm","","","","","","1050"]
["","","","Gylis","mm","","","","","","250"]
["Svoris","Įrenginys","","","kg","","","","","","12"]
["Ventiliatorius","Oro debitas","Aušinimas","Didelis","m³/min.","","","","","","16.0"]
["","","","Mažas","m³/min.","","","","","","11.3"]
["","","","Tylus veikimas","m³/min.","","","","","","10.1"]
["","","Šildymas","Didelis","m³/min.","","","","","","17.2"]
["","","","Mažas","m³/min.","","","","","","12.6"]
["","","","Tylus veikimas","m³/min.","","","","","","11.3"]
["Garso galingumo lygis","Vėsinimas","","","dBA","","","","","","60"]
["","Šildymas","","","dBA","","","","","","59"]
["Garso slėgio lygis","Aušinimas","","Aukštas","dBA","","","","","","45"]
["","","","Žemas","dBA","","","","","","36"]
["","","","Tylus veikimas","dBA","","","","","","33"]
["","Šildymas","","Aukštas","dBA","","","","","","44"]
["","","","Žemas","dBA","","","","","","35"]
["","","","Tylus veikimas","dBA","","","","","","32"]
["Vamzdžių jungtys","Skystis","","OD","mm","","","","","","6.35"]
["","Dujos","","Iš. diam.","mm","","","","","","12.7"]
["","Drenažas","","","","","","","","","18"]
["Valdymo sistemos","Nuotolinis infraraudonųjų spindulių pultelis","","","","","","","","","ARC452A3"]
["Standartiniai priedai","Installation manual","","","","","","","","","1"]
["","Wireless remote control","","","","","","","","","1"]
["","Operation manual","","","","","","","","","1"]
["","Batteries","","","","","","","","","2"]
["","Indoor unit fixing screws","","","","","","","","","2"]
["","Mounting plate","","","","","","","","","1"]
["","Remote control holder","","","","","","","","","1"]
["","Titanium apatite photocatalytic air purification filter","","","","","","","","","2"]
["El. tiekimas","Pavadinimas","","","","","","","","","V1"]
["","Fazė","","","","","","","","","1~"]
["Maitinimas","Dažnis","","","Hz","","","","","","50"]
["","Įtampa","","","V","","","","","","220-240"]
["Standartiniai priedai","Titano apatito fotokatalitinis oro gryninimo filtras be rėmo","","","","","","","","","","2"]
["Pastabos","","","","","","","","","","","(4) - 240 V"]