{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":48,"n_cols":11,"rows_kept":48,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXS-K / RXS-L"]
[]
[]
[]
[]
["","","","","FTXS20K2V1B / RXS20L2V1B","FTXS25K2V1B / RXS25L2V1B","FTXS35K2V1B / RXS35L2V1B","FTXS42K2V1B / RXS42L2V1B","FTXS42K3V1B / RXS42L2V1B","FTXS50K2V1B / RXS50L2V1B","FTXS50K3V1B / RXS50L2V1B"]
["Aušinimo galingumas","Min.","","kW","1.3","1.3","1.4","1.7","","1.7"]
["","Maks.","","kW","2.8","3.2","4.0","5.0","","5.3"]
["","Nom.","","kW","2.00","2.5","3.5","4.20","","5.00"]
["Vamzdžių jungtys","Skystis","OD","mm","6.35","6.35","6.35","6.35","","6.35"]
["","Dujos","Iš. diam.","mm","9.5","9.5","9.5","9.5","","12.7"]
["","Drenažo vamzdis","OD","mm","18","18","18","18","","18"]
["Vardinis našumas","Metinis energijos sunaudojimas","","kWh","215","285","430","590","","705"]
["","EER","","","4.65","4.39","4.07","3.56","","3.55"]
["","COP","","","4.72","4.67","4.76","4.12","","4.00"]
["","Energijos suvartojimo ženklinimo direktyva","Vėsinimas","","A","A","A","A","","A"]
["","","Šildymas","","A","A","A","A","","A"]
["Šildymo galingumas","Nom.","","kW","2.5","2.8","4.00","5.40","","5.80"]
["","Min.","","kW","1.3","1.3","1.4","1.7","","1.7"]
["","Maks.","","kW","4.3","4.7","5.2","6.0","","6.5"]
["Pastabos","","","","(1) - EER/COP pagal „Eurovent 2012“, skirta naudoti tik už ES ribų","(1) - EER/COP pagal „Eurovent 2012“, skirta naudoti tik už ES ribų","(1) - EER/COP pagal „Eurovent 2012“, skirta naudoti tik už ES ribų","(1) - EER/COP pagal „Eurovent 2012“, skirta naudoti tik už ES ribų","(1) - EER/COP pagal „Eurovent 2012“, skirta naudoti tik už ES ribų","(1) - EER/COP pagal „Eurovent 2012“, skirta naudoti tik už ES ribų","(1) - EER/COP pagal „Eurovent 2012“, skirta naudoti tik už ES ribų"]
["","","","","(2) - 220 V","(2) - 220 V","(2) - 220 V","(2) - 220 V","(2) - Nominalus efektyvumas: vėsinimas esant 35°/27° nominaliąja apkrova, šildymas esant 7°/20° nominaliąja apkrova","(2) - 220 V","(2) - Nominalus efektyvumas: vėsinimas esant 35°/27° nominaliąja apkrova, šildymas esant 7°/20° nominaliąja apkrova"]
["","","","","(3) - 230 V","(3) - 230 V","(3) - 230 V","(3) - 230 V","(3) - 220 V","(3) - 230 V","(3) - 220 V"]
["","","","","(4) - 240 V","(4) - 240 V","(4) - 240 V","(4) - 240 V","(4) - 230 V","(4) - 240 V","(4) - 230 V"]
["","","","","(5) - Nominalus efektyvumas: vėsinimas esant 35°/27° nominaliąja apkrova, šildymas esant 7°/20° nominaliąja apkrova","(5) - Nominalus efektyvumas: vėsinimas esant 35°/27° nominaliąja apkrova, šildymas esant 7°/20° nominaliąja apkrova","(5) - Nominalus efektyvumas: vėsinimas esant 35°/27° nominaliąja apkrova, šildymas esant 7°/20° nominaliąja apkrova","(5) - Nominalus efektyvumas: vėsinimas esant 35°/27° nominaliąja apkrova, šildymas esant 7°/20° nominaliąja apkrova","(5) - 240 V","(5) - Nominalus efektyvumas: vėsinimas esant 35°/27° nominaliąja apkrova, šildymas esant 7°/20° nominaliąja apkrova","(5) - 240 V"]
["Išorinis įrenginys","","","","","","","","RXS42L","","RXS50L"]
["Aušinimo galingumas","Min.","","kW","","","","","1.7","","1.7"]
["","Nom.","","kW","","","","","4.20","","5.00"]
["","Maks.","","kW","","","","","5.0","","5.3"]
["Šildymo galingumas","Min.","","kW","","","","","1.7","","1.7"]
["","Nom.","","kW","","","","","5.40","","5.80"]
["","Maks.","","kW","","","","","6.0","","6.5"]
["Nominalus efektyvumas","EER","","","","","","","3.35","","3.32"]
["","COP","","","","","","","4.12","","4.00"]
["","Metinis energijos sunaudojimas","","kWh","","","","","627","","753"]
["Vardinis našumas","Energijos suvartojimo ženklinimo direktyva","Vėsinimas","","","","","","A","","A"]
["","","Šildymas","","","","","","A","","A"]
["Vamzdžių jungtys","Drenažo vamzdis","OD","mm","","","","","18","","18"]
["","Dujos","Iš. diam.","mm","","","","","12.7","","12.7"]
["","Skystis","OD","mm","","","","","6.35","","6.35"]
["Patalpos vėsinimas","Energijos efektyvumo klasė","","","","","","","A++","","A++"]
["","Vėsinimas","Pdesign","kW","","","","","4.20","","5.00"]
["","SEER","","","","","","","6.80","","6.80"]
["","Metinės energijos sąnaudos","","kWh/m.","","","","","216","","257"]
["Patalpos šildymas (vidutinis klimatas)","Energijos efektyvumo klasė","","","","","","","A+","","A+"]
["","Pajėgumas","Pdesign","kW","","","","","4.00","","4.60"]
["","SCOP/A","","","","","","","4.20","","4.20"]
["","Metinės energijos sąnaudos","","kWh/m.","","","","","1334","","1535"]