{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":91,"n_cols":15,"rows_kept":91,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXS-K"]
[]
[]
[]
[]
["","","","","","FTXS20K2V1B","FTXS20K3V1B","FTXS25K2V1B","FTXS25K3V1B","FTXS35K2V1B","FTXS35K3V1B","FTXS42K2V1B","FTXS42K3V1B","FTXS50K2V1B","FTXS50K3V1B"]
["Garso slėgio lygis","Šildymas","","Aukštas","dBA","40","","","","","","45"]
["","","","Tylus veikimas","dBA","19","","","","","","22"]
["","","","Žemas","dBA","27","","","","","","33"]
["","Aušinimas","","Tylus veikimas","dBA","19","","","","","","21"]
["","","","Žemas","dBA","24","","","","","","33"]
["","","","Aukštas","dBA","40","","","","","","45"]
["","","","Nom.","dBA","34","","","","","","39"]
["","Aušinimas","","Nom.","dBA","32","","","","","","39"]
["Standartiniai priedai","Įrengimo vadovas","","","","1","","","","","","1"]
["","Eksploatavimo vadovas","","","","1","","","","","","1"]
["","Belaidis nuotolinis valdymas","","","","1","","","","","","1"]
["","Elementai","","","","2","","","","","","2"]
["","Nuotolinio valdymo pulto laikiklis","","","","1","","","","","","1"]
["","Pritvirtinimo plokštė","","","","1","","","","","","1"]
["","Vidinės įrangos pritvirtinimo varžtai","","","","2","","","","","","2"]
["","Titano apatito fotokatalizatoriaus oro gryninimo filtras","","","","2","","","","","","2"]
["Control systems","Infrared remote control","","","","ARC466A6","","","","","","ARC466A6"]
["Vamzdžių jungtys","Skystis","","OD","mm","6.35","","","","","","6.35"]
["","Dujos","","Iš. diam.","mm","9.5","","","","","","9.5"]
["","Drenažo vamzdis","","","","18","","","","","","18"]
["Tiekiama galia","Aušinimas","","Nom.","kW","0.04","","","","","","0.024 (2), 0.024 (3), 0.024 (4)"]
["","Šildymas","","Nom.","kW","0.04","","","","","","0.030 (2), 0.030 (3), 0.030 (4)"]
["Sound power level","Vėsinimas","","","dBA","58","","","","","","59"]
["","Šildymas","","","dBA","58","","","","","","59"]
["Matmenys","Vienetas","","Plotis","mm","780","","","","","","900"]
["","","","Gylis","mm","215","","","","","","215"]
["","","","Aukštis","mm","289","","","","","","298"]
["Korpusas","Spalva","","","","Balta spalva","","","","","","Balta spalva"]
["Svoris","Vienetas","","","kg","8","","","","","","11"]
["Power supply","Fazė","","","","1~","","","","","","1~"]
["","Dažnis","","","Hz","50","","","","","","50"]
["","Pavadinimas","","","","V1","","","","","","V1"]
["","Įtampa","","","V","220-240","","","","","","220-240"]
["Pastabos","","","","","(1) - 220 V","(1) - 220 V","(1) - 220 V","(1) - 220 V","(1) - 220 V","(1) - 220 V","(1) - Kai sujungtas su sudėtinės sistemos išoriniu įrenginiu, žr. sudėtinio išorinio įrenginio specifikacijas prie kurios jungsite.","(1) - 220 V","(1) - 220 V","(1) - 220 V"]
["","","","","","(2) - 230 V","(2) - 230 V","(2) - 230 V","(2) - 230 V","(2) - 230 V","(2) - 230 V","(2) - 220 V","(2) - 230 V","(2) - 230 V","(2) - 230 V"]
["","","","","","(3) - 240 V","(3) - 240 V","(3) - 240 V","(3) - 240 V","(3) - 240 V","(3) - 240 V","(3) - 230 V","(3) - 240 V","(3) - 240 V","(3) - 240 V"]
["Tiekiama galia","Aušinimas","","Nom.","kW","","0.040, 0.040, 0.040","0.04","0.040 (3) (1) (2), 0.040 (3) (1) (2), 0.040 (3) (1) (2)","0.026 (3) (4) (2), 0.026 (3) (4) (2), 0.026 (3) (4) (2)","0.026 (1) (3) (2), 0.026 (1) (3) (2), 0.026 (1) (3) (2)","","0.024, 0.024, 0.024","0.026 (4) (2) (3), 0.026 (4) (2) (3), 0.026 (4) (2) (3)","0.026 (1) (2) (3), 0.026 (1) (2) (3), 0.026 (1) (2) (3)"]
["","Šildymas","","Nom.","kW","","0.040, 0.040, 0.040","0.04","0.040 (2) (3) (1), 0.040 (2) (3) (1), 0.040 (2) (3) (1)","0.028 (2) (4) (3), 0.028 (2) (4) (3), 0.028 (2) (4) (3)","0.028 (1) (3) (2), 0.028 (1) (3) (2), 0.028 (1) (3) (2)","","0.030, 0.030, 0.030","0.032 (2) (4) (3), 0.032 (2) (4) (3), 0.032 (2) (4) (3)","0.032 (2) (1) (3), 0.032 (2) (1) (3), 0.032 (2) (1) (3)"]
["Korpusas","Spalva","","","","","Balta","Balta","Balta","Balta","Balta","","Balta","Balta","Balta"]
["Matmenys","Įrenginys","","Aukštis","mm","","215","289","215","298","215","","215","298","215"]
["","","","Plotis","mm","","780","780","780","900","900","","900","900","900"]
["","","","Gylis","mm","","289","215","289","215","298","","298","215","298"]
["Svoris","Įrenginys","","","kg","","8.00","8","8.00","11","11.0","","11.0","11","11.0"]
["Ventiliatorius","Oro debitas","Aušinimas","Didelis","m³/min.","","8.8","9.1","9.1","11.2","11.2","","11.2","11.9","11.9"]
["","Oro srauto greitis","Vėsinimas","Vidutinis","m³/min.","","6.7","7.0","7.0","","8.5","","9.1","","9.6"]
["","","","Mažas","m³/min.","","4.7","5.0","5.0","5.8","5.8","","7.0","7.4","7.4"]
["","","","Tylus veikimas","m³/min.","","3.9","3.9","3.9","4.1","4.1","","4.1","4.5","4.5"]
["","","Šildymas","Didelis","m³/min.","","9.5","10.0","10.0","12.1","12.1","","12.4","13.3","13.3"]
["","Oro srauto greitis","Šildymas","Vidutinis","m³/min.","","7.8","8.0","8.0","","9.3","","10.0","","10.8"]
["","","Šildymas","Mažas","m³/min.","","6.0","6.0","6.0","6.5","6.5","","7.8","8.4","8.4"]
["","","","Tylus veikimas","m³/min.","","4.3","4.3","4.3","4.2","4.2","","5.2","5.5","5.5"]
["Garso galingumo lygis","Vėsinimas","","","dBA","","58","58","58","59","59","","59","60","60"]
["","Šildymas","","","dBA","","58","58","58","59","59","","59","60","60"]
["Garso slėgio lygis","Aušinimas","","Aukštas","dBA","","40","41","41","45","45","","45","46","46"]
["","Vėsinimas","","Vidutinis","dBA","","32","33","33","","37","","39","","40"]
["","","","Žemas","dBA","","24","25","25","29","29","","33","34","34"]
["","","","Tylus veikimas","dBA","","19","19","19","19","19","","21","23","23"]
["","Šildymas","","Aukštas","dBA","","40","41","41","45","45","","45","47","47"]
["","","","Vidutinis","dBA","","34","34","34","","39","","39","","40"]
["","","","Žemas","dBA","","27","27","27","29","29","","33","34","34"]
["","","","Tylus veikimas","dBA","","19","19","19","19","19","","22","24","24"]
["Vamzdžių jungtys","Skystis","","OD","mm","","6.35","6.35","6.35","6.35","6.35","","6.35","6.35","6.35"]
["","Dujos","","Iš. diam.","mm","","9.50","9.5","9.50","9.5","9.50","","9.50","12.7","12.7"]
["","Drenažas","","","","","18","18","18","18","18","","18","18","18"]
["Control systems","Infrared remote control","","","","","ARC466A6","","","","","","ARC466A9"]
["Standartiniai priedai","Installation manual","","","","","1","1","1","1","1","","1","1","1"]
["","Wireless remote control","","","","","1","1","1","1","1","","1","1","1"]
["","AAA dry-cell batteries","","","","","2","","2","","2","","2","","2"]
["","Operation manual","","","","","1","1","1","1","1","","1","1","1"]
["","Titanium apatite deodorizing filter","","","","","2","","2","","2","","2","","2"]
["","Indoor unit fixing screws","","","","","2","2","2","2","2","","2","2","2"]
["","Mounting plate","","","","","1","1","1","1","1","","1","1","1"]
["","Remote control holder","","","","","1","1","1","1","1","","1","1","1"]
["El. tiekimas","Pavadinimas","","","","","V1","V1","V1","V1","V1","","V1","V1","V1"]
["","Fazė","","","","","1~","1~","1~","1~","1~","","1~","1~","1~"]
["Maitinimas","Dažnis","","","Hz","","50","50","50","50","50","","50","50","50"]
["","Įtampa","","","V","","220-240","220-240","220-240","220-240","220-240","","220-240","220-240","220-240"]
["Ventiliatorius","Oro debitas","Aušinimas","Nom.","m³/min.","","","9.1","","11.2","","","","11.9"]
["Garso slėgio lygis","Aušinimas","","Nom.","dBA","","","33","","37","","","","40"]
["Ventiliatorius","Oro debitas","Šildymas","Nom.","m³/min.","","","8.0","","9.3","","","","10.8"]
["Garso slėgio lygis","Šildymas","","Nom.","dBA","","","34","","39","","","","40"]
["Valdymo sistemos","Nuotolinis infraraudonųjų spindulių pultelis","","","","","","ARC466A6","ARC466A6","ARC466A6","ARC466A9","","","ARC466A6","ARC466A9"]
["Standartiniai priedai","Batteries","","","","","","2","","2","","","","2"]
["","Titanium apatite photocatalytic air purification filter","","","","","","2","","2","","","","2"]
["Pastabos","","","","","","","","","","","(4) - 240 V"]